{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["E.2 单项工程招标控制价投标报价汇总表(表-03)","E.3 单位工程招标控制价投标报价汇总表(表-04-1)一般~","F.1 分部分项工程和单价措施项目清单与计价表(表-08)【~","E.3 单位工程招标控制价投标报价汇总表(表-04-1)一~1","F.1 分部分项工程和单价措施项目清单与计价表(表-08)~1"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"E.2 单项工程招标控制价投标报价汇总表(表-03)","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"merged":[[0,0,0,5],[1,1,1,3],[1,4,1,5],[2,0,3,0],[2,1,3,1],[2,2,3,2],[2,3,2,5],[6,0,6,1]],"flags":["formulas_cached_only"]}
["单项工程招标控制价/投标报价汇总表","","","","",""]
["工程名称：","安居化工园区整体提升建设项目（管网工程）","","","",""]
["序号","单位工程名称 ","金额(元)","其中：（元）","",""]
["","","","暂估价","安全文明施工费 ","规费"]
["1","排水工程W1-W44段（含W44污水检查井）","2358323.65"," "," ","40457.82"]
["2","排水工程W44-W48（不含W44污水检查井）","2399225.33"," "," ","40527.29"]
["合　　计","","4757548.98"," "," ","80985.11"]

{"sheet":"E.3 单位工程招标控制价投标报价汇总表(表-04-1)一般~","index":1,"n_rows":21,"n_cols":5,"rows_kept":21,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,20,2]],"flags":["formulas_cached_only"]}
["单位工程招标控制价/投标报价汇总表","","","",""]
["（适用于一般计税方法）\r\n","","","",""]
["工程名称：","","安居化工园区整体提升建设项目（管网工程）W1-W44段（含W44污水检查井）","标段：/",""]
["序号","","汇总内容","金  额（元）","其中:暂估价(元)"]
["1","","分部分项及单价措施项目","2243389.57"," "]
["1.1","","管网工程","1504124.50"," "]
["1.2","","检查井","178779.43"," "]
["2","","总价措施项目"," ","-"]
["2.1","","其中：安全文明施工费"," ","-"]
["3","","其他项目"," ","-"]
["3.1","","其中：暂列金额"," ","-"]
["3.2","","其中：专业工程暂估价"," ","-"]
["3.3","","其中：计日工"," ","-"]
["3.4","","其中：总承包服务费"," ","-"]
["4","","规费","40457.82","-"]
["5","","创优质工程奖补偿奖励费"," ","-"]
["6","","税前不含税工程造价","2283847.39","-"]
["6.1","","其中：除税甲供材料（设备）费"," ","-"]
["7","","销项增值税额","68515.42","-"]
["8","","附加税","5960.84","-"]
[" 招标控制价/投标报价总价合计=税前不含税工程造价+销项增值税额+附加税","","","2358323.65"," "]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)【~","index":2,"n_rows":184,"n_cols":12,"rows_kept":184,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,1,41,2],[41,3,41,4],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[55,3,55,4],[56,1,56,2],[56,3,56,4],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[70,3,70,4],[71,1,71,2],[71,3,71,4],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[85,3,85,4],[86,1,86,2],[86,3,86,4],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[100,3,100,4],[101,1,101,2],[101,3,101,4],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[115,3,115,4],[116,1,116,2],[116,3,116,4],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[130,3,130,4],[131,1,131,2],[131,3,131,4],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[148,3,148,4],[149,1,149,2],[149,3,149,4],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[166,3,166,4],[167,1,167,2],[167,3,167,4],[168,1,168,2],[168,3,168,4],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[182,3,182,4],[183,0,183,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","安居化工园区整体提升建设项目（管网工程）W1-W44段（含W44污水检查井）】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","管网工程 ",""," "," "," "," "," "," "," "]
["1","040102002001","","挖沟槽石方","1.土壤类别：详见地勘报告或说明\n2.挖土深度：综合考虑\n3.运输距离：施工方自行考虑，综合单价已考虑回填场内倒运，费用不另记取\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","18026.66","8.95","161338.61","30825.59","96983.43",""]
["2","040101002002","","挖沟槽土方","1.土壤类别：详见地勘报告或说明\n2.挖土深度：综合考虑\n3.运输距离：施工方自行考虑，综合单价已考虑回填方场内倒运，费用不另记取\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","54079.99","7.60","411007.92","78415.99","246604.75",""]
["3","040103001003","","回填土","1.密实度要求：详设计图纸\n2.填方材料品种：详设计图纸\n3.填方粒径要求：详设计图纸\n4.填方来源、运距：现场土石方进行回填 运距综合考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","62176.48","6.37","396064.18","72746.48","239379.45",""]
["4","040103002004","","余方弃置","1.废弃料品种：土石方综合考虑\n2.运距：施工方自行考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","9930.17","6.50","64546.11","11916.20","38926.27",""]
["5","040501001005","","HDPE中空壁塑钢缠绕管sn12.5 d1400","1.HDPE中空壁塑钢缠绕管sn12.5 d1400 \n2.管座材质：详见设计图纸\n3.规格：d1400 \n4.接口方式：承插\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","898.94","91.29","82064.23","44569.45","9519.77",""]
["6","040501001006","","HDPE中空壁塑钢缠绕管sn12.5 d800","1.HDPE中空壁塑钢缠绕管sn12.5 d800 \n2.管座材质：详见设计图纸\n3.规格：d800 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","25","30.03","750.75","392.25","101.75",""]
["7","040501001007","","HDPE中空壁塑钢缠绕管sn12.5 d600","1.HDPE中空壁塑钢缠绕管sn12.5 d600 \n2.管座材质：详见设计图纸\n3.规格：d600 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.以包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1452","24.59","35704.68","21315.36","1916.64",""]
["8","040501001008","","HDPE中空壁塑钢缠绕管sn12.5 d500","1.HDPE中空壁塑钢缠绕管sn12.5 d500 \n2.管座材质：详见设计图纸\n3.规格：d500 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","8","20.68","165.44","98.88","8.80",""]
["9","040501001009","","HDPE中空壁塑钢缠绕管sn12.5 d400","1.HDPE中空壁塑钢缠绕管sn12.5 d400 \n2.管座材质：详见设计图纸\n3.规格：d400 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","10","15.66","156.60","92.90","8.80",""]
["10","040303001010","","管道混凝土基础","1.混凝土强度等级：C25商品混凝土\n2.尺寸：详设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3739.5","58.61","219172.10","139146.80","822.69",""]
["11","040305001011","","软基换填","1.砂夹卵石垫层\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","612.29","88.98","54481.56","32273.81","3539.04",""]
["12","040501001012","","污水专线管保护 混凝土包管","1.混凝土强度等级：C25商品混凝土\n2.尺寸：详做法详图S-10\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","270.38","84.94","22966.08","14516.70","116.26",""]
["13","010515002013","","预制砼调节环钢筋 φ8","1.预制砼调节环钢筋 φ8\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.159","5520.23","877.72","164.96","18.23",""]
["14","010514002014","","预制砼调节环 C40","1.预制砼调节环安装\n2.材质，厚度：C40混凝土\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","1.53","289.09","442.31","260.07","0.11",""]
["15","040303002015","","检查井加固","1.检查井井周加固\n2.材料：6%水泥稳定碎石，分层夯实到最佳密实度98%以上\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","348.62","69.30","24159.37","15199.83","610.09",""]
["16","041001001016","","拆除滨江路沥青路面","1.拆除滨江路道路沥青路面\n2.材质，厚度：5cm厚细粒式改性沥青混凝AC-13C+7cm厚中粒式密级配普通沥青混凝土AC-20C\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2675.45","3.60","9631.62","3451.33","4815.81",""]
["17","041001003017","","拆除滨江路道路基层","1.拆除滨江路道路基层\n2.材质，厚度：20cm厚5%水泥稳定级配碎石基层+20cm 4%水泥稳定级配碎石底基层+15cm级配碎石垫层\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","1169","9.60","11222.40","3039.40","6710.06",""]
["18","041001001018","","拆除厂区道路面层","1.拆除厂区道路面层\n2.材质，厚度：22cm厚C35混凝土\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","100","7.06","706.00","234.00","375.00",""]
["19","041001003019","","拆除厂区道路基层","1.拆除厂区道路基层\n2.材质，厚度：20cm厚5%水泥稳定级配碎石基层+15cm级配碎石垫层\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","100","6.11","611.00","165.00","365.00",""]
["20","041001007020","","拆除厂区围墙","1.拆除厂区围墙\n2.建筑垃圾运距距离：施工方根据现场情况自行考虑\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m","10","24.15","241.50","196.20","",""]
["21","040203003021","","喷粘结油PC-3 乳化沥青","1.PC-3 乳化沥青\n2.喷油量0.7~1.5kg/m2\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["22","040203003022","","喷透层油PC-2 乳化沥青","1.PC-2 乳化沥青\n2.喷油量 0.3~0.6kg/m2\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["23","040203006023","","7cm厚中粒式密级配普通沥青混凝土AC-20C","1.恢复沥青混凝土路面\n2.材质规格，厚度：7cm厚中粒式密级配普通沥青混凝土AC-20C\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["24","040203006024","","5cm厚细粒式改性沥青混凝AC-13C","1.恢复沥青混凝土路面\n2.材质规格，厚度：5cm厚细粒式改性沥青混凝AC-13C\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["25","040202015025","","20cm厚5%水泥稳定级配碎石基层","1.恢复滨江路道路基层\n2.材质规格，厚度：20cm厚5%水泥稳定级配碎石基层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["26","040202015026","","20cm 4%水泥稳定级配碎石底基层","1.恢复滨江路道路基层\n2.材质规格，厚度：20cm 4%水泥稳定级配碎石底基层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["27","040203007027","","22cm厚C35混凝土路面","1.恢复厂区道路面层\n2.材质，厚度：22cm厚C35混凝土\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m2","100","14.35","1435.00","910.00","7.00",""]
["28","040202015028","","15cm级配碎石垫层","1.恢复滨江路道路基层\n2.材质规格，厚度：15cm级配碎石垫层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["29","011503001029","","金属扶手、栏杆、栏板","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","11.7","233.48","2731.72","924.07","40.13",""]
["30","010501001030","","垫层混凝土 C15","1.部位：围墙\n2.混凝土种类 商品混凝土 C15\n3.做法参照12J003-F6-1\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","0.8","482.25","385.80","32.87","0.20",""]
["31","011204003031","","块料墙面","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","10","115.89","1158.90","589.40","0.10",""]
["32","011407001032","","墙面喷刷涂料","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","21.84","20.31","443.57","217.74","",""]
["33","040305004033","","砖围墙","1.恢复厂区围墙\n2.做法参照12J003-F6-1\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.5","663.73","1659.33","465.05","0.80",""]
[" "," ","","分部小计 ",""," "," "," ","1504124.50","472160.33","650870.18"," "]
[" "," ","","检查井 ",""," "," "," "," "," "," "," "]
[" "," ","","1900mm*1100mm矩形混凝土污水检查井（14座） ",""," "," "," "," "," "," "," "]
["34","040601007034","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","51.24","73.80","3781.51","2381.12","14.35",""]
["35","040601006035","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","14.84","56.24","834.60","523.41","4.16",""]
["36","040601010036","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","25.9","70.70","1831.13","1144.52","7.25",""]
["37","040504005037","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","21","462.50","9712.50","288.12","304.92",""]
["38","040601012038","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","14","54.72","766.08","444.78","9.10",""]
["39","040303001039","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","6.58","43.72","287.68","179.77","1.38",""]
["40","040901001040","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","9.562","1224.01","11703.98","6445.46","883.72",""]
["41","010606008041","","成品塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","140","4.81","673.40","257.60","",""]
["42","070205001042","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","14","679.77","9516.78","362.04","0.56",""]
["43","041102028043","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","317.97","49.48","15733.16","7421.42","184.42",""]
["44","041102029044","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","21.28","70.68","1504.07","675.85","28.09",""]
["45","041102030045","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","26.6","43.49","1156.83","622.17","22.08",""]
["46","041102001046","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","11.76","30.15","354.56","199.57","3.29",""]
[" "," ","","分部小计 ",""," "," "," ","57856.28","20945.83","1463.32"," "]
[" "," ","","2400mm*2400mm矩形混凝土污水检查井（3座） ",""," "," "," "," "," "," "," "]
["47","040601007047","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","29.16","73.80","2152.01","1355.07","8.16",""]
["48","040601006048","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","9.21","56.24","517.97","324.84","2.58",""]
["49","040601010049","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","4.47","70.70","316.03","197.53","1.25",""]
["50","040504005050","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","4.5","462.50","2081.25","61.74","65.34",""]
["51","040601012051","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","30.18","54.72","1651.45","958.82","19.62",""]
["52","040303001052","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.27","43.72","142.96","89.34","0.69",""]
["53","040901001053","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","5.94","1224.01","7270.62","4003.98","548.97",""]
["54","010606008054","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","30","8.41","252.30","55.20","",""]
["55","070205001055","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","3","679.77","2039.31","77.58","0.12",""]
["56","041102028056","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","208.42","49.48","10312.62","4864.52","120.88",""]
["57","041102030057","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","10.08","43.49","438.38","235.77","8.37",""]
["58","041102029058","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","6.72","70.68","474.97","213.43","8.87",""]
["59","041102001059","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","3.6","30.15","108.54","61.09","1.01",""]
[" "," ","","分部小计 ",""," "," "," ","27758.41","12498.91","785.86"," "]
[" "," ","","2700mm*2700mm矩形混凝土污水检查井（0座） ",""," "," "," "," "," "," "," "]
["60","040601007060","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["61","040601006061","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["62","040601010062","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["63","040504005063","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["64","040601012064","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["65","040303001065","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["66","040901001066","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["67","010606008067","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","0"," ","","","",""]
["68","070205001068","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["69","041102028069","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["70","041102030070","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["71","041102029071","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["72","041102001072","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
[" "," ","","分部小计 ",""," "," "," "," "," "," "," "]
[" "," ","","Φ1000圆形混凝土污水检查井（28座） ",""," "," "," "," "," "," "," "]
["73","040601007073","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","48.72","73.80","3595.54","2264.02","13.64",""]
["74","040601006074","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","11.2","56.24","629.89","395.02","3.14",""]
["75","040601010075","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","4.76","70.70","336.53","210.34","1.33",""]
["76","040504005076","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","42","462.50","19425.00","576.24","609.84",""]
["77","040601012077","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","4.2","54.72","229.82","133.43","2.73",""]
["78","040303001078","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","6.44","43.72","281.56","175.94","1.35",""]
["79","040901001079","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","5.32","1224.01","6511.73","3586.05","491.67",""]
["80","010606008080","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","168","8.41","1412.88","309.12","",""]
["81","070205001081","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","28","679.77","19033.56","724.08","1.12",""]
["82","041102028082","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","519.09","49.48","25684.57","12115.56","301.07",""]
["83","041102030083","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","24.61","43.49","1070.29","575.63","20.43",""]
["84","041102029084","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","19.69","70.68","1391.69","625.35","25.99",""]
["85","041102001085","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","28.14","30.15","848.42","477.54","7.88",""]
[" "," ","","分部小计 ",""," "," "," ","80451.48","22168.32","1480.19"," "]
[" "," ","","Φ1250圆形混凝土污水检查井（0座） ",""," "," "," "," "," "," "," "]
["86","040601007086","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["87","040601006087","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["88","040601010088","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["89","040504005089","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["90","040601012090","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["91","040303001091","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["92","040901001092","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["93","010606008093","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","0"," ","","","",""]
["94","070205001094","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["95","041102028095","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["96","041102030096","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["97","041102029097","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["98","041102001098","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
[" "," ","","分部小计 ",""," "," "," "," "," "," "," "]
[" "," ","","Φ1400圆形混凝土污水检查井（2座） ",""," "," "," "," "," "," "," "]
["99","040601007099","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","10.98","73.80","810.32","510.24","3.07",""]
["100","040601006100","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.34","56.24","187.84","117.80","0.94",""]
["101","040601010101","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.68","70.70","189.48","118.43","0.75",""]
["102","040504005102","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","3","462.50","1387.50","41.16","43.56",""]
["103","040601012103","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","4.86","54.72","265.94","154.40","3.16",""]
["104","040303001104","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.44","43.72","62.96","39.34","0.30",""]
["105","040901001105","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.502","1224.01","614.45","338.38","46.39",""]
["106","010606008106","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","20","4.81","96.20","36.80","",""]
["107","070205001107","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","2","679.77","1359.54","51.72","0.08",""]
["108","041102028108","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","143.26","49.48","7088.50","3343.69","83.09",""]
["109","041102030109","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","6.44","43.49","280.08","150.63","5.35",""]
["110","041102029110","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","4.29","70.68","303.22","136.25","5.66",""]
["111","041102001111","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2.23","30.15","67.23","37.84","0.62",""]
[" "," ","","分部小计 ",""," "," "," ","12713.26","5076.68","192.97"," "]
[" "," ","","Φ1400圆形混凝土污水检查井(超深井)（0座） ",""," "," "," "," "," "," "," "]
["112","040601007112","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["113","040601006113","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["114","040601010114","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["115","040504005115","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["116","040601012116","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["117","040303001117","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["118","040901001118","","现浇构件钢筋 直径（mm） φ≤10","1.钢筋种类、规格 现浇构件钢筋 直径（mm） φ≤10\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["119","040901001119","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["120","040901001120","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ＞16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ＞16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["121","010606008121","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","0"," ","","","",""]
["122","070205001122","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["123","070205001123","","玻璃钢格栅盖板900*900","1.玻璃钢格栅盖板900*900\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["124","041102028124","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["125","041102030125","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["126","041102029126","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["127","041102001127","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
[" "," ","","分部小计 ",""," "," "," "," "," "," "," "]
[" "," ","","Φ1600圆形混凝土污水检查井(超深井)（0座） ",""," "," "," "," "," "," "," "]
["128","040601007128","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["129","040601006129","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["130","040601010130","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["131","040504005131","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["132","040601012132","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["133","040303001133","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0"," ","","","",""]
["134","040901001134","","现浇构件钢筋 直径（mm） φ≤10","1.钢筋种类、规格 现浇构件钢筋 直径（mm） φ≤10\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["135","040901001135","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["136","040901001136","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ＞16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ＞16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0"," ","","","",""]
["137","010606008137","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","0"," ","","","",""]
["138","070205001138","","玻璃钢格栅盖板900*900","1.玻璃钢格栅盖板900*900\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["139","070205001139","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","0"," ","","","",""]
["140","041102028140","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["141","041102030141","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["142","041102029142","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["143","041102001143","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
[" "," ","","分部小计 ",""," "," "," "," "," "," "," "]
[" "," ","","分部小计 ",""," "," "," ","178779.43","60689.74","3922.34"," "]
[" "," ","","单价措施项目清单 ",""," "," "," "," "," "," "," "]
["144","041106001001","","履带式挖掘机进出场及安拆","1.机械设备名称 履带式挖掘机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","1","3567.88","3567.88","1170.00","1572.07",""]
["145","041106001002","","锚杆钻孔机进出场及安拆","1.机械设备名称 锚杆钻孔机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","0"," ","","","",""]
["146","041106001003","","钢板桩打桩机进出场及安拆","1.机械设备名称 钢板桩打桩机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","0"," ","","","",""]
["147","041102001001","","管道包封模板","1.管道包封模板\n2.模板类型：综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","8834.53","60.29","532633.81","299843.95","4947.34",""]
["148","041101005001","","检查井脚手架 1900mm*1100mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：1900mm*1100mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","998.2","10.69","10670.76","3952.87","259.53",""]
["149","041101005002","","检查井脚手架 2400mm*2400mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：2400mm*2400mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","283.2","10.69","3027.41","1121.47","73.63",""]
["150","041101005003","","检查井脚手架 2700mm*2700mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：2700mm*2700mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["151","041101005004","","检查井脚手架 Φ1000圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1000圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","871.46","10.69","9315.91","3450.98","226.58",""]
["152","041101005005","","检查井脚手架 Φ1250圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1250圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["153","041101005006","","检查井脚手架 Φ1400圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","113.15","10.69","1209.57","448.07","29.42",""]
["154","041101005007","","检查井脚手架 Φ1400圆形混凝土污水检查井(超深井)","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井(超深井)\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["155","041101005008","","检查井脚手架 Φ1600圆形混凝土污水检查井(超深井)","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井(超深井)\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["156","041102001","","围墙垫层模板","1.围墙垫层模板\n2.模板类型：综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2","30.15","60.30","33.94","0.56",""]
[" "," ","","分部小计 ",""," "," "," ","560485.64","310021.28","7109.13"," "]
["合    计","","","","","","","","2243389.57","842871.35","661901.65",""]

{"sheet":"E.3 单位工程招标控制价投标报价汇总表(表-04-1)一~1","index":3,"n_rows":21,"n_cols":5,"rows_kept":21,"merged":[[0,0,0,4],[1,0,1,4],[2,0,2,1],[3,0,3,1],[4,0,4,1],[5,0,5,1],[6,0,6,1],[7,0,7,1],[8,0,8,1],[9,0,9,1],[10,0,10,1],[11,0,11,1],[12,0,12,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[16,0,16,1],[17,0,17,1],[18,0,18,1],[19,0,19,1],[20,0,20,2]],"flags":["formulas_cached_only"]}
["单位工程招标控制价/投标报价汇总表","","","",""]
["（适用于一般计税方法）\r\n","","","",""]
["工程名称：","","安居化工园区整体提升建设项目（管网工程）W44-W48段（不含W44污水检查井）","标段：/",""]
["序号","","汇总内容","金  额（元）","其中:暂估价(元)"]
["1","","分部分项及单价措施项目","2282930.10"," "]
["1.1","","管网工程","1614180.24"," "]
["1.2","","检查井","275934.23"," "]
["2","","总价措施项目"," ","-"]
["2.1","","其中：安全文明施工费"," ","-"]
["3","","其他项目"," ","-"]
["3.1","","其中：暂列金额"," ","-"]
["3.2","","其中：专业工程暂估价"," ","-"]
["3.3","","其中：计日工"," ","-"]
["3.4","","其中：总承包服务费"," ","-"]
["4","","规费","40527.29","-"]
["5","","创优质工程奖补偿奖励费"," ","-"]
["6","","税前不含税工程造价","2323457.39","-"]
["6.1","","其中：除税甲供材料（设备）费"," ","-"]
["7","","销项增值税额","69703.72","-"]
["8","","附加税","6064.22","-"]
[" 招标控制价/投标报价总价合计=税前不含税工程造价+销项增值税额+附加税","","","2399225.33"," "]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)~1","index":4,"n_rows":184,"n_cols":12,"rows_kept":184,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[39,3,39,4],[40,1,40,2],[40,3,40,4],[41,1,41,2],[41,3,41,4],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[55,3,55,4],[56,1,56,2],[56,3,56,4],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[70,3,70,4],[71,1,71,2],[71,3,71,4],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[85,3,85,4],[86,1,86,2],[86,3,86,4],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[100,3,100,4],[101,1,101,2],[101,3,101,4],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[109,1,109,2],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[115,3,115,4],[116,1,116,2],[116,3,116,4],[117,1,117,2],[118,1,118,2],[119,1,119,2],[120,1,120,2],[121,1,121,2],[122,1,122,2],[123,1,123,2],[124,1,124,2],[125,1,125,2],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[130,3,130,4],[131,1,131,2],[131,3,131,4],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[148,3,148,4],[149,1,149,2],[149,3,149,4],[150,1,150,2],[151,1,151,2],[152,1,152,2],[153,1,153,2],[154,1,154,2],[155,1,155,2],[156,1,156,2],[157,1,157,2],[158,1,158,2],[159,1,159,2],[160,1,160,2],[161,1,161,2],[162,1,162,2],[163,1,163,2],[164,1,164,2],[165,1,165,2],[166,1,166,2],[166,3,166,4],[167,1,167,2],[167,3,167,4],[168,1,168,2],[168,3,168,4],[169,1,169,2],[170,1,170,2],[171,1,171,2],[172,1,172,2],[173,1,173,2],[174,1,174,2],[175,1,175,2],[176,1,176,2],[177,1,177,2],[178,1,178,2],[179,1,179,2],[180,1,180,2],[181,1,181,2],[182,1,182,2],[182,3,182,4],[183,0,183,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","安居化工园区整体提升建设项目（管网工程）W44-W48段（不含W44污水检查井）】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","管网工程 ",""," "," "," "," "," "," "," "]
["1","040102002001","","挖沟槽石方","1.土壤类别：详见地勘报告或说明\n2.挖土深度：综合考虑\n3.运输距离：施工方自行考虑，综合单价已考虑回填场内倒运，费用不另记取\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","18026.66","8.95","161338.61","30825.59","96983.43",""]
["2","040101002002","","挖沟槽土方","1.土壤类别：详见地勘报告或说明\n2.挖土深度：综合考虑\n3.运输距离：施工方自行考虑，综合单价已考虑回填方场内倒运，费用不另记取\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","54079.99","7.60","411007.92","78415.99","246604.75",""]
["3","040103001003","","回填土","1.密实度要求：详设计图纸\n2.填方材料品种：详设计图纸\n3.填方粒径要求：详设计图纸\n4.填方来源、运距：现场土石方进行回填 运距综合考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","62176.48","6.37","396064.18","72746.48","239379.45",""]
["4","040103002004","","余方弃置","1.废弃料品种：土石方综合考虑\n2.运距：施工方自行考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","9930.17","6.50","64546.11","11916.20","38926.27",""]
["5","040501001005","","HDPE中空壁塑钢缠绕管sn12.5 d1400","1.HDPE中空壁塑钢缠绕管sn12.5 d1400 \n2.管座材质：详见设计图纸\n3.规格：d1400 \n4.接口方式：承插\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","2514.06","91.29","229508.54","124647.09","26623.90",""]
["6","040501001006","","HDPE中空壁塑钢缠绕管sn12.5 d800","1.HDPE中空壁塑钢缠绕管sn12.5 d800 \n2.管座材质：详见设计图纸\n3.规格：d800 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["7","040501001007","","HDPE中空壁塑钢缠绕管sn12.5 d600","1.HDPE中空壁塑钢缠绕管sn12.5 d600 \n2.管座材质：详见设计图纸\n3.规格：d600 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.以包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["8","040501001008","","HDPE中空壁塑钢缠绕管sn12.5 d500","1.HDPE中空壁塑钢缠绕管sn12.5 d500 \n2.管座材质：详见设计图纸\n3.规格：d500 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["9","040501001009","","HDPE中空壁塑钢缠绕管sn12.5 d400","1.HDPE中空壁塑钢缠绕管sn12.5 d400 \n2.管座材质：详见设计图纸\n3.规格：d400 \n4.接口方式：承插接口\n5.采用HDPE中空壁塑钢缠绕管sn12.5，详见设计图纸\n6.已包含闭水试验等其他完成此项工作费用\n7.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","0"," ","","","",""]
["10","040303001010","","管道混凝土基础","1.混凝土强度等级：C25商品混凝土\n2.尺寸：详设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3739.5","58.61","219172.10","139146.80","822.69",""]
["11","040305001011","","软基换填","1.砂夹卵石垫层\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","612.29","88.98","54481.56","32273.81","3539.04",""]
["12","040501001012","","污水专线管保护 混凝土包管","1.混凝土强度等级：C25商品混凝土\n2.尺寸：详做法详图S-10\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","270.38","84.94","22966.08","14516.70","116.26",""]
["13","010515002013","","预制砼调节环钢筋 φ8","1.预制砼调节环钢筋 φ8\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.159","1676.87","266.62","164.96","18.23",""]
["14","010514002014","","预制砼调节环 C40","1.预制砼调节环安装\n2.材质，厚度：C40混凝土\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","1.53","289.09","442.31","260.07","0.11",""]
["15","040303002015","","检查井加固","1.检查井井周加固\n2.材料：6%水泥稳定碎石，分层夯实到最佳密实度98%以上\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","348.62","69.30","24159.37","15199.83","610.09",""]
["16","041001001016","","拆除滨江路沥青路面","1.拆除滨江路道路沥青路面\n2.材质，厚度：5cm厚细粒式改性沥青混凝AC-13C+7cm厚中粒式密级配普通沥青混凝土AC-20C\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2675.45","3.60","9631.62","3451.33","4815.81",""]
["17","041001003017","","拆除滨江路道路基层","1.拆除滨江路道路基层\n2.材质，厚度：20cm厚5%水泥稳定级配碎石基层+20cm 4%水泥稳定级配碎石底基层+15cm级配碎石垫层\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","1169","9.60","11222.40","3039.40","6710.06",""]
["18","041001001018","","拆除厂区道路面层","1.拆除厂区道路面层\n2.材质，厚度：22cm厚C35混凝土\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","100","7.06","706.00","234.00","375.00",""]
["19","041001003019","","拆除厂区道路基层","1.拆除厂区道路基层\n2.材质，厚度：20cm厚5%水泥稳定级配碎石基层+15cm级配碎石垫层\n3.综合单价包含切缝等为完成此项工作的其他工作\n4.建筑垃圾运距距离：施工方根据现场情况自行考虑\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","100","6.11","611.00","165.00","365.00",""]
["20","041001007020","","拆除厂区围墙","1.拆除厂区围墙\n2.建筑垃圾运距距离：施工方根据现场情况自行考虑\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m","10","24.15","241.50","196.20","",""]
["21","040203003021","","喷粘结油PC-3 乳化沥青","1.PC-3 乳化沥青\n2.喷油量0.7~1.5kg/m2\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["22","040203003022","","喷透层油PC-2 乳化沥青","1.PC-2 乳化沥青\n2.喷油量 0.3~0.6kg/m2\n3.其他：详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["23","040203006023","","7cm厚中粒式密级配普通沥青混凝土AC-20C","1.恢复沥青混凝土路面\n2.材质规格，厚度：7cm厚中粒式密级配普通沥青混凝土AC-20C\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["24","040203006024","","5cm厚细粒式改性沥青混凝AC-13C","1.恢复沥青混凝土路面\n2.材质规格，厚度：5cm厚细粒式改性沥青混凝AC-13C\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["25","040202015025","","20cm厚5%水泥稳定级配碎石基层","1.恢复滨江路道路基层\n2.材质规格，厚度：20cm厚5%水泥稳定级配碎石基层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["26","040202015026","","20cm 4%水泥稳定级配碎石底基层","1.恢复滨江路道路基层\n2.材质规格，厚度：20cm 4%水泥稳定级配碎石底基层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["27","040203007027","","22cm厚C35混凝土路面","1.恢复厂区道路面层\n2.材质，厚度：22cm厚C35混凝土\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m2","100","14.35","1435.00","910.00","7.00",""]
["28","040202015028","","15cm级配碎石垫层","1.恢复滨江路道路基层\n2.材质规格，厚度：15cm级配碎石垫层\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0"," ","","","",""]
["29","011503001029","","金属扶手、栏杆、栏板","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","11.7","233.48","2731.72","924.07","40.13",""]
["30","010501001030","","垫层混凝土 C15","1.部位：围墙\n2.混凝土种类 商品混凝土 C15\n3.做法参照12J003-F6-1\n4.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范\n","m3","0.8","482.25","385.80","32.87","0.20",""]
["31","011204003031","","块料墙面","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","10","115.89","1158.90","589.40","0.10",""]
["32","011407001032","","墙面喷刷涂料","1.做法参照12J003-F6-1\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","21.84","20.31","443.57","217.74","",""]
["33","040305004033","","砖围墙","1.恢复厂区围墙\n2.做法参照12J003-F6-1\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.5","663.73","1659.33","465.05","0.80",""]
[" "," ","","分部小计 ",""," "," "," ","1614180.24","530338.58","665938.32"," "]
[" "," ","","检查井 ",""," "," "," "," "," "," "," "]
[" "," ","","1900mm*1100mm矩形混凝土污水检查井（30座） ",""," "," "," "," "," "," "," "]
["34","040601007034","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","109.8","73.80","8103.24","5102.41","30.74",""]
["35","040601006035","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","31.8","56.24","1788.43","1121.59","8.90",""]
["36","040601010036","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","55.5","517.92","28744.56","2452.55","15.54",""]
["37","040504005037","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","45","462.50","20812.50","617.40","653.40",""]
["38","040601012038","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","30","54.72","1641.60","953.10","19.50",""]
["39","040303001039","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","14.1","43.72","616.45","385.21","2.96",""]
["40","040901001040","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","20.49","1224.01","25079.96","13811.69","1893.69",""]
["41","010606008041","","成品塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","300","4.81","1443.00","552.00","",""]
["42","070205001042","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","30","679.77","20393.10","775.80","1.20",""]
["43","041102028043","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","681.36","49.48","33713.69","15902.94","395.19",""]
["44","041102029044","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","45.6","70.68","3223.01","1448.26","60.19",""]
["45","041102030045","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","57","43.49","2478.93","1333.23","47.31",""]
["46","041102001046","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","25.2","30.15","759.78","427.64","7.06",""]
[" "," ","","分部小计 ",""," "," "," ","148798.25","44883.82","3135.68"," "]
[" "," ","","2400mm*2400mm矩形混凝土污水检查井（2座） ",""," "," "," "," "," "," "," "]
["47","040601007047","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","19.44","73.80","1434.67","903.38","5.44",""]
["48","040601006048","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","6.14","56.24","345.31","216.56","1.72",""]
["49","040601010049","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.98","70.70","210.69","131.69","0.83",""]
["50","040504005050","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","3","462.50","1387.50","41.16","43.56",""]
["51","040601012051","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","20.12","54.72","1100.97","639.21","13.08",""]
["52","040303001052","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.18","43.72","95.31","59.56","0.46",""]
["53","040901001053","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","3.96","1224.01","4847.08","2669.32","365.98",""]
["54","010606008054","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","20","8.41","168.20","36.80","",""]
["55","070205001055","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","2","679.77","1359.54","51.72","0.08",""]
["56","041102028056","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","138.94","49.48","6874.75","3242.86","80.59",""]
["57","041102030057","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","6.72","43.49","292.25","157.18","5.58",""]
["58","041102029058","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","4.48","70.68","316.65","142.28","5.91",""]
["59","041102001059","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2.4","30.15","72.36","40.73","0.67",""]
[" "," ","","分部小计 ",""," "," "," ","18505.28","8332.45","523.90"," "]
[" "," ","","2700mm*2700mm矩形混凝土污水检查井（1座） ",""," "," "," "," "," "," "," "]
["60","040601007060","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","11.44","73.80","844.27","531.62","3.20",""]
["61","040601006061","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.68","56.24","206.96","129.79","1.03",""]
["62","040601010062","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.92","70.70","135.74","84.84","0.54",""]
["63","040504005063","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1.5","462.50","693.75","20.58","21.78",""]
["64","040601012064","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1","54.72","54.72","31.77","0.65",""]
["65","040303001065","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1","43.72","43.72","27.32","0.21",""]
["66","040901001066","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","2.296","1224.01","2810.33","1547.66","212.20",""]
["67","010606008067","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","10","8.41","84.10","18.40","",""]
["68","070205001068","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","1","679.77","679.77","25.86","0.04",""]
["69","041102028069","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","76.9","49.48","3805.01","1794.85","44.60",""]
["70","041102030070","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","3.96","43.49","172.22","92.62","3.29",""]
["71","041102029071","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2.48","70.68","175.29","78.76","3.27",""]
["72","041102001072","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","1.4","30.15","42.21","23.76","0.39",""]
[" "," ","","分部小计 ",""," "," "," ","9748.09","4407.83","291.20"," "]
[" "," ","","Φ1000圆形混凝土污水检查井（1座） ",""," "," "," "," "," "," "," "]
["73","040601007073","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.74","73.80","128.41","80.86","0.49",""]
["74","040601006074","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.4","56.24","22.50","14.11","0.11",""]
["75","040601010075","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.17","70.70","12.02","7.51","0.05",""]
["76","040504005076","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1.5","462.50","693.75","20.58","21.78",""]
["77","040601012077","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.15","54.72","8.21","4.77","0.10",""]
["78","040303001078","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.23","43.72","10.06","6.28","0.05",""]
["79","040901001079","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.19","1224.01","232.56","128.07","17.56",""]
["80","010606008080","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","6","8.41","50.46","11.04","",""]
["81","070205001081","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","1","679.77","679.77","25.86","0.04",""]
["82","041102028082","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","18.54","49.48","917.36","432.72","10.75",""]
["83","041102030083","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0.88","43.49","38.27","20.58","0.73",""]
["84","041102029084","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0.7","70.68","49.48","22.23","0.92",""]
["85","041102001085","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","1.01","30.15","30.45","17.14","0.28",""]
[" "," ","","分部小计 ",""," "," "," ","2873.30","791.75","52.86"," "]
[" "," ","","Φ1250圆形混凝土污水检查井（1座） ",""," "," "," "," "," "," "," "]
["86","040601007086","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.13","73.80","157.19","98.98","0.60",""]
["87","040601006087","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.54","56.24","30.37","19.05","0.15",""]
["88","040601010088","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.3","70.70","21.21","13.26","0.08",""]
["89","040504005089","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1.5","462.50","693.75","20.58","21.78",""]
["90","040601012090","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.33","54.72","18.06","10.48","0.21",""]
["91","040303001091","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","0.3","43.72","13.12","8.20","0.06",""]
["92","040901001092","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.226","1224.01","276.63","152.34","20.89",""]
["93","010606008093","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","6","4.81","28.86","11.04","",""]
["94","070205001094","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","1","679.77","679.77","25.86","0.04",""]
["95","041102028095","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","22.4","49.48","1108.35","522.82","12.99",""]
["96","041102030096","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","1.04","43.49","45.23","24.33","0.86",""]
["97","041102029097","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0.93","70.68","65.73","29.54","1.23",""]
["98","041102001098","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","0.58","30.15","17.49","9.84","0.16",""]
[" "," ","","分部小计 ",""," "," "," ","3155.76","946.32","59.05"," "]
[" "," ","","Φ1400圆形混凝土污水检查井（6座） ",""," "," "," "," "," "," "," "]
["99","040601007099","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","32.94","73.80","2430.97","1530.72","9.22",""]
["100","040601006100","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","10.02","56.24","563.52","353.41","2.81",""]
["101","040601010101","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","8.04","70.70","568.43","355.29","2.25",""]
["102","040504005102","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","9","462.50","4162.50","123.48","130.68",""]
["103","040601012103","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","14.58","54.72","797.82","463.21","9.48",""]
["104","040303001104","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","4.32","43.72","188.87","118.02","0.91",""]
["105","040901001105","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","1.505","1224.01","1842.14","1014.48","139.09",""]
["106","010606008106","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","60","4.81","288.60","110.40","",""]
["107","070205001107","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","6","679.77","4078.62","155.16","0.24",""]
["108","041102028108","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","429.78","49.48","21265.51","10031.07","249.27",""]
["109","041102030109","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","19.31","43.49","839.79","451.66","16.03",""]
["110","041102029110","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","12.87","70.68","909.65","408.75","16.99",""]
["111","041102001111","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","6.68","30.15","201.40","113.36","1.87",""]
[" "," ","","分部小计 ",""," "," "," ","38137.82","15229.01","578.84"," "]
[" "," ","","Φ1400圆形混凝土污水检查井(超深井)（1座） ",""," "," "," "," "," "," "," "]
["112","040601007112","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","27.12","73.80","2001.46","1260.27","7.59",""]
["113","040601006113","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.96","56.24","110.23","69.13","0.55",""]
["114","040601010114","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.13","70.70","79.89","49.93","0.32",""]
["115","040504005115","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1.5","462.50","693.75","20.58","21.78",""]
["116","040601012116","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.5","54.72","82.08","47.66","0.98",""]
["117","040303001117","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","1.3","43.72","56.84","35.52","0.27",""]
["118","040901001118","","现浇构件钢筋 直径（mm） φ≤10","1.钢筋种类、规格 现浇构件钢筋 直径（mm） φ≤10\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.065","1651.95","107.38","66.75","1.95",""]
["119","040901001119","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.331","1224.01","405.15","223.12","30.59",""]
["120","040901001120","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ＞16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ＞16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","10.239","1334.88","13667.84","6462.24","2221.66",""]
["121","010606008121","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","23","4.81","110.63","42.32","",""]
["122","070205001122","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","1","679.77","679.77","25.86","0.04",""]
["123","070205001123","","玻璃钢格栅盖板900*900","1.玻璃钢格栅盖板900*900\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","2","49.97","99.94","38.02","0.08",""]
["124","041102028124","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","56.91","49.48","2815.91","1328.28","33.01",""]
["125","041102030125","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","7.9","43.49","343.57","184.78","6.56",""]
["126","041102029126","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","3","70.68","212.04","95.28","3.96",""]
["127","041102001127","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2.68","30.15","80.80","45.48","0.75",""]
[" "," ","","分部小计 ",""," "," "," ","21547.28","9995.22","2330.09"," "]
[" "," ","","Φ1600圆形混凝土污水检查井(超深井)（1座） ",""," "," "," "," "," "," "," "]
["128","040601007128","","井壁混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","53.74","73.80","3966.01","2497.30","15.05",""]
["129","040601006129","","井底混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.86","56.24","217.09","136.14","1.08",""]
["130","040601010130","","井顶混凝土","1.混凝土强度等级：C30P6\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","2.27","70.70","160.49","100.31","0.64",""]
["131","040504005131","","预制混凝土井筒安装","1.预制混凝土井筒安装 φ700\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m","1.5","462.50","693.75","20.58","21.78",""]
["132","040601012132","","流槽(C15) 商品混凝土","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.36","54.72","183.86","106.75","2.18",""]
["133","040303001133","","混凝土垫层","1.混凝土强度等级：C15\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m3","3.29","43.72","143.84","89.88","0.69",""]
["134","040901001134","","现浇构件钢筋 直径（mm） φ≤10","1.钢筋种类、规格 现浇构件钢筋 直径（mm） φ≤10\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.12","1651.95","198.23","123.24","3.60",""]
["135","040901001135","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ12～16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ12～16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","0.388","1224.01","474.92","261.54","35.86",""]
["136","040901001136","","现浇构件钢筋 高强钢筋（屈服强度≥400） φ＞16","1.钢筋种类、规格 高强钢筋（屈服强度≥400） φ＞16\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","t","15.657","1334.88","20900.22","9881.76","3397.26",""]
["137","010606008137","","塑钢踏步","1.踏步材质、规格：爬梯采用塑钢成品\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","个","23","4.81","110.63","42.32","",""]
["138","070205001138","","玻璃钢格栅盖板900*900","1.玻璃钢格栅盖板900*900\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","2","49.97","99.94","38.02","0.08",""]
["139","070205001139","","铸铁井盖","1.盖板材质、规格：新型五防球墨铸铁井盖，安全网已包含在主材价格中不单另记取。\n2.井盖、井圈材质及规格：详见设计图纸\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","块","1","679.77","679.77","25.86","0.04",""]
["140","041102028140","","井壁（隔墙）模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","89.75","49.48","4440.83","2094.77","52.06",""]
["141","041102030141","","底板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","8","43.49","347.92","187.12","6.64",""]
["142","041102029142","","顶板模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","6.72","70.68","474.97","213.43","8.87",""]
["143","041102001143","","垫层模板","1.模板类型：综合考虑\n2.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2.52","30.15","75.98","42.76","0.71",""]
[" "," ","","分部小计 ",""," "," "," ","33168.45","15861.78","3546.54"," "]
[" "," ","","分部小计 ",""," "," "," ","275934.23","100448.18","10518.16"," "]
[" "," ","","单价措施项目清单 ",""," "," "," "," "," "," "," "]
["144","041106001001","","履带式挖掘机进出场及安拆","1.机械设备名称 履带式挖掘机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","1","3567.88","3567.88","1170.00","1572.07",""]
["145","041106001002","","锚杆钻孔机进出场及安拆","1.机械设备名称 锚杆钻孔机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","0"," ","","","",""]
["146","041106001003","","钢板桩打桩机进出场及安拆","1.机械设备名称 钢板桩打桩机\n2.机械设备规格型号 综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","台次","0"," ","","","",""]
["147","041102001001","","管道包封模板","1.管道包封模板\n2.模板类型：综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","11748.73","30.15","354224.21","199375.95","3289.64",""]
["148","041101005001","","检查井脚手架 1900mm*1100mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：1900mm*1100mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2139","10.69","22865.91","8470.44","556.14",""]
["149","041101005002","","检查井脚手架 2400mm*2400mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：2400mm*2400mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","188.8","10.69","2018.27","747.65","49.09",""]
["150","041101005003","","检查井脚手架 2700mm*2700mm矩形混凝土污水检查井","1.脚手架搭拆\n2.部位：2700mm*2700mm矩形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","119.54","10.69","1277.88","473.38","31.08",""]
["151","041101005004","","检查井脚手架 Φ1000圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1000圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","100.55","10.69","1074.88","398.18","26.14",""]
["152","041101005005","","检查井脚手架 Φ1250圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1250圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","61.35","10.69","655.83","242.95","15.95",""]
["153","041101005006","","检查井脚手架 Φ1400圆形混凝土污水检查井","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","339.46","10.69","3628.83","1344.26","88.26",""]
["154","041101005007","","检查井脚手架 Φ1400圆形混凝土污水检查井(超深井)","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井(超深井)\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","136.35","10.69","1457.58","539.95","35.45",""]
["155","041101005008","","检查井脚手架 Φ1600圆形混凝土污水检查井(超深井)","1.脚手架搭拆\n2.部位：Φ1400圆形混凝土污水检查井(超深井)\n3.脚手架材质:钢管、竹、木支架、爬升设备等综合\n4.本项目投标人应根据设计图、施工组织设计、现场实际情况综合报价，不论采用何种搭设方式该综合单价结算不作调整\n5.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","185.6","10.69","1984.06","734.98","48.26",""]
["156","041102001","","围墙垫层模板","1.围墙垫层模板\n2.模板类型：综合考虑\n3.其他未尽事宜详见设计图纸，满足技术规范、现行施工验收规范","m2","2","30.15","60.30","33.94","0.56",""]
[" "," ","","分部小计 ",""," "," "," ","392815.63","213531.68","5712.64"," "]
["合    计","","","","","","","","2282930.1","844318.44","682169.12",""]