{"text_format":"3","workbook":"xls","n_sheets":11,"sheets":["C.2 工程项目招标工程量清单扉页(扉-2)","汇总表","D 工程计价总说明(表-01)","F.1 分部分项工程和单价措施项目清单与计价表(表-08)【~","K.2 承包人提供主要材料和工程设备一览表(表-20)【B-~","F.1 分部分项工程和单价措施项目清单与计价表(表-08)~1","K.2 承包人提供主要材料和工程设备一览表(表-20)【B~1","F.1 分部分项工程和单价措施项目清单与计价表(表-08)~2","K.2 承包人提供主要材料和工程设备一览表(表-20)【B~2","F.1 分部分项工程和单价措施项目清单与计价表(表-08)~3","K.2 承包人提供主要材料和工程设备一览表(表-20)【B~3"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"C.2 工程项目招标工程量清单扉页(扉-2)","index":0,"n_rows":13,"n_cols":8,"rows_kept":13,"merged":[[0,1,0,5],[0,6,0,7],[1,0,1,7],[2,0,2,2],[2,3,2,6],[3,0,4,2],[3,3,4,6],[3,7,4,7],[5,0,5,1],[5,2,5,3],[5,5,5,7],[6,0,6,1],[6,2,6,3],[6,5,6,7],[7,0,7,1],[7,2,7,3],[7,5,7,7],[8,0,8,1],[8,2,8,3],[8,5,8,7],[9,0,9,1],[9,2,9,3],[9,5,9,7],[10,0,10,1],[10,2,10,3],[10,5,10,7],[11,0,11,1],[11,2,11,3],[11,5,11,7],[12,0,12,7]],"flags":["formulas_cached_only"]}
["","遂宁市安居区东城二期棚户区改造项目","","","","","工程",""]
["一标段劳务招标工程量清单","","","","","","",""]
["招标控制价(小写):","","",10768596.66,"","","",""]
["(大写):","","",10768596.66,"","","",""]
["","","","","","","",""]
["招　标　人:","",null,null,"造价咨询人:"]
["","","(单位盖章)","","","(单位盖章)","",""]
["法定代表人 \r\n或其授权人:","",null,null,"法定代表人 \r\n或其授权人:"]
["       ","","(签字或盖章)","","","(签字或盖章)","",""]
["编　制　人:","",null,null,"复　核　人:"]
["","","(造价人员签字盖专用章)","","","(一级造价工程师签字盖专用章)","",""]
["     编 制 时 间:","",null,null,"复 核 时 间:"," ","",""]
["扉-2 ","","","","","","",""]

{"sheet":"汇总表","index":1,"n_rows":11,"n_cols":10,"rows_kept":11,"merged":[[0,0,0,9],[1,0,2,0],[1,1,2,1],[1,2,2,2],[1,3,2,6],[1,7,2,7],[1,8,2,8],[1,9,2,9],[3,1,9,1],[3,2,9,2],[3,3,5,3],[3,5,5,5],[3,8,5,8],[6,3,8,3],[6,5,6,6],[6,7,6,8],[7,5,7,6],[7,7,7,8],[8,5,8,6],[8,7,8,8],[9,3,9,6],[9,7,9,8],[10,0,22,9]],"flags":["formulas_cached_only"]}
["遂宁市安居区东城二期棚户区改造项目劳务（一标段）招标工程量清单"]
["序号","楼号","建筑面积（㎡）","费用组成",{"$nulls":3},"金额（元）","合计（元）","备注"]
[]
[1,"1号楼",14704.55,"可竞争费","⑴","人材机直接费用","人工费含调差(元)",8337888.47,10768596.66]
[2,{"$nulls":3},"⑵",null,"辅材费(元)",2106800.17]
[3,{"$nulls":3},"⑶",null,"机械费(元)",323908.02]
[4,null,null,"不可竞争费","⑷","规费",null,"四川省2020清单计价规范Ⅳ档施工专业承包劳务分包资质4.8%计取"]
[5,{"$nulls":3},"⑸","安全文明施工费",null,"建筑面积*25元/㎡"]
[6,{"$nulls":3},"⑹","税金",null,"（⑴+⑵+⑶+⑷+⑸）*3%"]
[7,null,null,"暂定合同总价",{"$nulls":3},"⑴+⑵+⑶+⑷+⑸+⑹"]
["说明：\n1、本次劳务招标范围：1#楼±0.000以上；\n2、土建工程除：防水保温、门窗幕墙以外的全部施工项；\n3、安装工程招标范围：强弱电工程、给排水工程；\n4、以上需招标工程周转铺材详见各栋材料表；\n5、规费按四川省2020清单计价规范Ⅳ档施工专业承包劳务分包资质4.8%计取；\n6、安全文明施工费按建筑面积25元/㎡计取；（包括但不限于：工人的安全防护用品、安全文明施工警示标志牌、垃圾清运、施工现场材料存放设施、安全检测费、临时设施、洞口和临边防护设施、消防设施与消防器材、安全教育培训费用、其他安全防护措施费用、场地硬化、楼梯边防护、现场安全管理人员、电气保护、安全照明设施、临水临电等其他文明施工环保措施，项目部按相关要求对各栋进行安全文明施工进行考核，最终安全文明施工费=建筑面积*25元/㎡*考核得分）\n7、税金按增值税3%计取。\n8、本次招标综合单价为未下浮综合单价，如本项目实施过程中有工程量增减或新增，按此计算：原综合单价*(1-N%)=新综合单价，N为劳务公司投标下浮百分率。"]

{"sheet":"D 工程计价总说明(表-01)","index":2,"n_rows":4,"n_cols":3,"rows_kept":4,"merged":[[0,0,0,2],[2,0,3,2]],"flags":["formulas_cached_only"]}
["总 说 明","",""]
["工程名称：","遂宁市安居区东城二期棚户区改造项目",""]
["1.工程概况：\r\n  项目名称：遂宁市安居区东城二期棚户区改造项目\r\n  建设地点：遂宁市安居区。\r\n  场地概况：遂宁市安居区，交通便利，用地平整，形状为略不规则条状地块，周边配套设施完善。\r\n2.工程招标和专业工程发包范围：\r\n   详招标文件、工程量清单及施工图所示全部内容。\r\n3.工程量清单编制依据：\r\n  3.1、本工程设计施工图、相关规范及配套图集；\r\n  3.2、常规施工办法及其他有关的施工及验收规范、标准、技术资料； \r\n  3.3、中华人民共和国国家标准《建设工程工程量清单计价规范》（GB50500-2013）及其配套文件、2020年《四川省建设工程工程量清单计价定额》及其配套文件； \r\n  3.4、材料价格按照《四川省工程造价信息》2023年第4期(2023年3月)遂宁市安居区信息价及遂宁市发布的2023年4月地区信息价；信息价缺项部分参考遂宁市及周边城市信息价和市场价)； \r\n  3.5、《四川省建设工程安全文明施工费计价管理办法》；\r\n  3.6、人工费调整按四川省建设工程造价管理总站关于对各市、州2020年《四川省建设工程工程量清单计价定额》人工费调整的批复（川建价发〔2022〕33号）执行；\r\n  3.7、《四川省住房和城乡建设厅印发关于重新调整<建筑业营业税改征增值税四川省建设工程计价依据调整办法>的通知（川建造价发〔2019〕181号）》。 \r\n4.工程质量、材料、施工等的特殊要求 \r\n  4.1、工程质量应达到国家现有质量验收标准； \r\n  4.2、材料品质和规格必须符合设计和规范要求，材料需见证取样并经检测合格。\r\n5.其他需要说明的问题：\r\n  5.1、工程量清单所列的工程量是按照施工设计图计算的，仅作为合同清单的基础，竣工结算按实际完成工程量，实际完成工程量的计算方式按照中华人民共和国国家标准《建设工程工程量清单计价规范》（GB50500-2013）及其配套文件和2020《四川省建设工程工程量清单计价定额》及相关配套文件进行计算；\r\n  5.2、工程量清单中项目的做法详见施工图设计或通用图集，清单项目特征与设计图如存在不一致均以设计图为准。各项目综合单价应包括设计图、相应标准图集和清单中规定的所有工序工作内容的全部费用；\r\n  5.3、清单项目特征仅列主要特征，其余特征详见设计图纸及图纸引用的标准图集和相关规范执行；\r\n  5.4、实际施工过程中与本工程量清单特征有变更的，按招标文件、合同约定的调整办法执行；\r\n  5.5、环境保护费、文明施工费、安全施工费、临时设施费费率按建筑与装饰工程基本费费率加现场评价费最高费率计列； \r\n  5.6、规费按“规费费率计取表”中Ⅰ档费率计算；\r\n  5.7、本工程混凝土均采用商品混凝土，砂浆采用预拌砂浆，商品混凝土泵送费、运输费用等全部费用计入综合单价中，结算不作调整；\r\n  5.8、本工程螺纹钢均采用抗震钢筋钢材牌号带“E”进行考虑；\r\n  5.9、马凳筋工程量根据一般施工方案进行计算；\r\n  5.10、PVC成品滴水、门窗洞口细部处理、地漏及管道周边细部处理、女儿墙根部的圆弧处理等在各项目的综合单价中予以考虑，不再单独列项计算；\r\n  5.11、砼楼板无论是收光还是拉毛均综合考虑，不因施工做法调整而进行费用的调整；\r\n  5.12、绿化成活养护期:乔木1年、灌木6个月、地被植物及草皮3个月；\r\n  5.13、地上的砼挡水均采用C25砼；\r\n  5.14、根据实际施工情况，地下室侧壁不考虑用3:7灰土回填；\r\n  5.15、依据地勘资料，地下室部分的桩长按照14m/根计算、幼儿园桩长按照20m/根计算；\r\n  5.16、根据实际施工情况，取消天棚抹灰，同时考虑梁板的清水模板费用；\r\n  5.17、人防密闭房间考虑同设备管井做法；地上封闭百叶内的墙面及天棚按照刮腻子考虑；\r\n  5.18、钢筋的工程量，均按照设计图纸及通常施工工艺的连接方式考虑后计算；\r\n  5.19、本次预算不包括高低压供配电系统和发电机组；\r\n  5.20、主体的大型机械设备进出场及安拆均统一考虑在各地块的地下室建筑与装饰工程的单价措施项目中，投标人应根据工程实际需要进行投标报价。\r\n\r\n\r\n","",""]
["","",""]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)【~","index":3,"n_rows":157,"n_cols":12,"rows_kept":157,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[13,3,13,4],[14,1,14,2],[14,3,14,4],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[46,3,46,4],[47,1,47,2],[47,3,47,4],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[52,3,52,4],[53,1,53,2],[53,3,53,4],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[68,3,68,4],[69,1,69,2],[69,3,69,4],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[79,3,79,4],[80,1,80,2],[80,3,80,4],[81,1,81,2],[82,1,82,2],[83,1,83,2],[83,3,83,4],[84,1,84,2],[84,3,84,4],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[94,3,94,4],[95,1,95,2],[95,3,95,4],[96,1,96,2],[97,1,97,2],[97,3,97,4],[98,1,98,2],[98,3,98,4],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[107,1,107,2],[108,1,108,2],[108,3,108,4],[109,1,109,2],[109,3,109,4],[110,1,110,2],[111,1,111,2],[112,1,112,2],[113,1,113,2],[114,1,114,2],[115,1,115,2],[116,1,116,2],[117,1,117,2],[118,1,118,2],[119,1,119,2],[119,3,119,4],[120,1,120,2],[120,3,120,4],[121,1,121,2],[121,3,121,4],[122,1,122,2],[123,1,123,2],[124,1,124,2],[124,3,124,4],[125,1,125,2],[125,3,125,4],[126,1,126,2],[127,1,127,2],[128,1,128,2],[129,1,129,2],[130,1,130,2],[131,1,131,2],[132,1,132,2],[133,1,133,2],[134,1,134,2],[135,1,135,2],[136,1,136,2],[137,1,137,2],[138,1,138,2],[139,1,139,2],[140,1,140,2],[141,1,141,2],[142,1,142,2],[143,1,143,2],[144,1,144,2],[145,1,145,2],[146,1,146,2],[147,1,147,2],[148,1,148,2],[148,3,148,4],[149,1,149,2],[149,3,149,4],[150,1,150,2],[151,1,151,2],[151,3,151,4],[152,1,152,2],[152,3,152,4],[153,1,153,2],[154,1,154,2],[154,3,154,4],[155,1,155,2],[155,3,155,4],[156,0,156,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【建筑与装饰工程】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","0104 砌筑工程 ",""," "," "," "," "," "," "," "]
["1","010401003003","","页岩实心砖墙 H≤3.6m","1.墙体类型:页岩实心砖墙\n2.墙体厚度:综合\n3.砖品种、规格、强度等级:页岩实心砖，强度、规格综合\n4.砂浆强度等级、配合比:M5干混砌筑砂浆\n5.按图集及规范要求墙脚、墙顶、洞口侧等部位需配砌的页岩实心砖（配砖规格综合）等费用综合考虑进入本项综合单价之中","m3","366.52","249.78"]
["2","010401004005","","页岩多孔砖墙 H≤3.6m","1.墙体类型:页岩多孔砖墙\n2.墙体厚度:综合\n3.砖品种、规格、强度等级:页岩多孔砖，强度、规格综合\n4.砂浆强度等级、配合比:M5干混砌筑砂浆\n5.按图集及规范要求墙脚、墙顶、洞口侧等部位需配砌的页岩实心砖（配砖规格综合）等费用综合考虑进入本项综合单价之中","m3","1703.97","249.78"]
["3","010401004006","","页岩多孔砖墙 H＞3.6m","1.墙体类型:页岩多孔砖墙\n2.墙体厚度:综合\n3.砖品种、规格、强度等级:页岩多孔砖，强度、规格综合\n4.砂浆强度等级、配合比:M5干混砌筑砂浆\n5.按图集及规范要求墙脚、墙顶、洞口侧等部位需配砌的页岩实心砖（配砖规格综合）等费用综合考虑进入本项综合单价之中","m3","15.01","324.24"]
["4","010401012004","","屋面出入口","1.砖品种、规格、强度等级:页岩实心砖，规格综合\n2.砂浆强度等级、配合比：M5水泥砂浆砌筑\n3.C15砼\n4.30mm厚M20水泥豆石面层、密封膏嵌缝\n5.其他：包含按设计、图集及规范需完成本项目的所有相关工作内容","个","2","91.04"]
["5","010401012005","","变形缝处踏步","1.砖品种、规格、强度等级:页岩实心砖，规格综合\n2.砂浆强度等级、配合比：M5水泥砂浆砌筑\n3.20mm厚M20聚合物水泥砂浆面层\n4.其他：包含按设计、图集及规范需完成本项目的所有相关工作内容","个","1","218.67"]
["6","010507003003","","排水沟","1.100厚C10混凝土垫层\n2.C15砼找坡（最薄处30mm）\n3.M5水泥砂浆砌砖暗沟\n4.20厚1:2.5水泥砂浆加5%防水剂抹面\n5.铸铁落水篦子，上盖土工布\n6..综合单价含土方挖、运、填、盖板等全部工作内容\n7.具体详见设计大样图","m","266.05","89.65"]
["7","070202001003","","厨房排烟道","1.采用钢丝网增强水泥排油烟气道\n2.烟道截面形状、长度:详国标16J916-1\n3.安装要求:包含安装、勾缝、楼板处封堵、烟道止回阀、风帽、防虫网等所有工作内容，此项费用综合考虑进入本项综合单价\n4.其它:烟道应满足设计、规范及相关文件的要求","m","568","63.42"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0105 混凝土及钢筋混凝土工程 ",""," "," "," "]
["8","010502001003","","矩形柱 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","6.4","65.05"]
["9","010502002003","","构造柱 C25","1.混凝土种类：细石商品混凝土 \n2.混凝土强度等级：C25\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.4.包含构造柱、门框、边框\n5.其他：满足设计、施工及验收规范要求\n","m3","269.45","92.85"]
["10","010503002003","","矩形梁 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","10.27","51.51"]
["11","010503004005","","圈梁及现浇带 C25","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C25\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","12.01","85.73"]
["12","010503004006","","翻边、挡水及门槛 C25","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C25\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","57.65","85.73"]
["13","010503005003","","过梁 C25","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C25\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.综合考虑预制及现浇构件\n5.其他：满足设计、施工及验收规范要求","m3","25.8","90.01"]
["14","010504001007","","直形墙 C40","1.混凝土种类：商品混凝土 \n2.混凝土强度等级：C40\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.清单工程量包含暗柱、暗梁、连梁\n5.其他：满足设计、施工及验收规范要求","m3","323.69","69.68"]
["15","010504001008","","直形墙 C35","1.混凝土种类：商品混凝土 \n2.混凝土强度等级：C35\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.清单工程量包含暗柱、暗梁、连梁\n5.其他：满足设计、施工及验收规范要求","m3","449.99","69.68"]
["16","010504001009","","直形墙 C30","1.混凝土种类：商品混凝土 \n2.混凝土强度等级：C30\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.清单工程量包含暗柱、暗梁、连梁\n5.其他：满足设计、施工及验收规范要求","m3","1882.46","69.68"]
["17","010504004003","","屋面挡墙 C15","1.混凝土种类：商品混凝土 \n2.混凝土强度等级：C15\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","10.37","69.68"]
["18","010505001005","","商品砼节点高强砼 C40","1.混凝土种类：商品砼\n2.混凝土强度等级：C40\n3.混凝土拌合料：投标人投标报价时应综合考虑砼骨料粒径及外加剂的相关费用，并满足设计及施工验收规范要求\n4.其它：商品砼的运输及泵送方式等由投标人综合考虑到投标报价中","m3","41.49","53.08"]
["19","010505001006","","有梁板 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","2434.95","53.08"]
["20","010505003003","","平板 C20","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C20\n3.混凝土拌合料:骨料粒径综合且满足设计及施工验收规范要求\n4.综合单价含砼的泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n5.其他：满足设计和规范要求","m3","1.31","61.49"]
["21","010505008003","","悬挑板 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.混凝土拌合料:骨料粒径综合且满足设计及施工验收规范要求\n4.综合单价含砼的泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n5.综合考虑悬挑板、雨棚板、凸窗板\n6.其他：满足设计和规范要求","m3","236.82","51.51"]
["22","010505006003","","凸窗侧板 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.混凝土拌合料:骨料粒径综合且满足设计及施工验收规范要求\n4.综合单价含砼的泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n5.其他：满足设计和规范要求","m3","106.83","69.68"]
["23","010507005003","","压顶 C25","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C25\n3.混凝土拌合料:骨料粒径综合且满足设计及施工验收规范要求\n4.综合单价含砼的泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n5.其他：满足设计和规范要求","m3","4.96","51.51"]
["24","010506001003","","直形楼梯 C30","1.混凝土种类：商品混凝土\n2.混凝土强度等级：C30\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m2","270.5","45.17"]
["25","010507001003","","散水","1.素土夯实\n2.150mm厚5-32粒径卵石灌M2.5混合砂浆垫层\n3.60mm厚C20混凝土提浆抹面\n4.250mm厚滤水性强种植土\n5.建筑油膏嵌缝\n6.具体详见设计","m2","288.74","12.69"]
["26","010507007003","","其他构件 C20","1.混凝土种类：细石商品混凝土\n2.混凝土强度等级：C20\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","6.34","116.74"]
["27","010508001003","","管井后浇板 C35","1.混凝土种类：补偿收缩商品混凝土\n2.混凝土强度等级：C35\n3.综合单价含砼的外加剂费用和泵送（含电费、油费、水费等）费用，不因运输泵送方式不同而调整单价\n4.其他：满足设计、施工及验收规范要求","m3","21.18","86.17"]
["28","010512001003","","预制板 C25","1.坡屋面用预制板C25，80mm厚含钢筋\n2.吊装及安装费用综合考虑，结算不作调整","m3","35.53","392.26"]
["29","010515001018","","砌体加筋 HPB300 直径φ6～φ10","1.钢筋种类、规格：热轧光圆钢筋  HPB300 Φ6~10\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求","t","13.277","1471.74"]
["30","010515001019","","现浇构件钢筋 HPB300 直径φ6~10","1.钢筋种类、规格：热轧光圆钢筋  HPB300 Φ6~10\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求","t","20.362","1471.74"]
["31","010515001020","","现浇构件钢筋 HRB400E 直径φ6~10","1.钢筋种类、规格：热轧带肋钢筋  HRB400E φ6~10\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求\n","t","359.415","1471.74"]
["32","010515001021","","现浇构件钢筋 HRB400E 直径φ12～φ14","1.钢筋种类、规格：热轧带肋钢筋  HRB400E φ12~14\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋（构造柱除外）或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求","t","178.661","1536.10"]
["33","010515001022","","现浇构件钢筋 HRB400E 直径φ16","1.钢筋种类、规格：热轧带肋钢筋  HRB400E φ16\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求\n","t","39.419","1536.10"]
["34","010515001023","","现浇构件钢筋 HRB400E 直径φ18～φ22","1.钢筋种类、规格：热轧带肋钢筋 HRB400E φ18~22\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求\n","t","67.856","1563.50"]
["35","010515001024","","现浇构件钢筋 HRB400E 直径φ25","1.钢筋种类、规格：热轧带肋钢筋 HRB400E φ25\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接或机械连接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求","t","8.572","1563.50"]
["36","010515001025","","支撑钢筋（铁马）","1.钢筋种类、规格：综合\n2.综合考虑钢筋埋设的方式，无论采用预留、植筋（除设计注明外）或其他方式施工，其所有费用均包括在所报综合单价中不再另行计取\n3.弧形构件钢筋增加费用在综合单价内综合考虑，结算时不做调整\n4.钢筋的调直、绑扎、焊接等费用在综合单价内综合考虑，结算时不做调整\n5.其他：满足设计、施工及验收规范要求","t","6.004","1471.74"]
["37","010515001026","","植筋 φ12","1.材料种类：钢筋 \n2.材料规格：φ12\n3.植入深度：满足设计及相关规范要求\n4.植筋胶品种：满足设计及相关规范要求","m","3194.88","42.60"]
["38","010516002003","","预埋铁件","1.部位：水沟、电缆沟等角钢、扁钢、钢板预埋件，以及其他清单项目中未列出的部位\n2.钢材种类、规格：详设计综合\n3.铁件尺寸：详设计综合\n4.油漆品种、刷漆遍数：预埋件外露部分的防腐、涂刷油漆综合考虑，颜色、质感满足业主及设计要求，费用不作调整\n5.其他：满足设计、施工及验收规范要求","t","1.587","2886.68"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0106 金属结构工程 ",""," "," "," "]
["39","010606008005","","屋面检修梯","1.钢材品种、规格:详见设计图\n2.油漆品种、刷漆遍数:详见设计图\n3.制作、安装、运输、吊装、填塞、埋件等完成此项工作的所有费用均包含在综合单价中\n4.具体做法详见设计图及西南图集18J201-119-2","t","0.074","8437.87"]
["40","010606008006","","屋面钢楼梯","1.钢材品种、规格:详见设计图\n2.油漆品种、刷漆遍数:详见设计图\n3.制作、安装、运输、吊装、填塞、埋件等完成此项工作的所有费用均包含在综合单价中\n4.具体样式及做法应根据建设单位使用及规范要求予以深化设计，综合考虑在投标报价中","t","3.6","8372.13"]
["41","010607005003","","砌块墙钢丝网加固","1.材料品种、规格：镀锌钢丝网(丝径、孔径、镀锌综合)\n2.加固方式：综合考虑\n3.其他：满足设计、施工及验收规范要求","m2","9455.33","11.10"]
["42","010607006003","","梁柱节点金属网","1.材料品种、规格：镀锌钢丝网(丝径、孔径、镀锌综合)\n2.加固方式：综合考虑\n3.部位：后浇带、梁柱砼相交且砼标号级差2级及以上位置\n3.其他：满足设计、施工及验收规范要求","m2","56.46","12.29"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0111 楼地面装饰工程 ",""," "," "," "]
["43","011101001011","","水泥砂浆楼面 架空层楼1","1.20mm厚M15水泥砂浆找平层\n2.2mm厚JS防水涂料（清单另列）\n3.20厚M20水泥砂浆面层铁板赶光\n4.其余满足设计要求","m2","179.41","26.47"]
["44","011101001012","","水泥砂浆楼面 楼5","1.水泥浆一道（内掺建筑胶）\n2.M15水泥防水砂浆找平层兼找坡，最薄处20mm厚\n3.JS防水涂料（清单另列）\n4.20厚M20水泥砂浆\n4.其余满足设计要求","m2","931.97","27.65"]
["45","011101001013","","水泥砂浆楼面 楼6","1.20厚M20水泥砂浆\n2.其余满足设计要求","m2","7860.65","12.81"]
["46","011101001014","","水泥砂浆楼面 楼7","1.20厚M15水泥砂浆\n2.其余满足设计要求","m2","220.8","12.81"]
["47","011101001015","","水泥砂浆楼面 空调百叶内地面","1.水泥浆一道（内掺建筑胶）\n2.M20水泥防水砂浆坡向地漏或出水口，最薄处≥20mm厚\n3.JS防水涂料（清单另列）\n4.20厚M20水泥砂浆\n5.其余满足设计要求","m2","450.36","33.76"]
["48","011101003005","","细石混凝土楼地面 楼4","1.水泥浆一道（内掺建筑胶）\n2.40mm厚C25细石砼面层，表面撒1:1水泥石子随打随抹光\n3.其余满足设计要求","m2","21.12","15.67"]
["49","011102003006","","800*800防滑波化砖楼面 楼1","1.水泥浆一道（内掺建筑胶）\n2.20厚M20水泥砂浆\n3.800*800mm玻化通体砖（防滑），勾缝\n4.其余满足设计要求\n","m2","1241.84","43.00"]
["50","011102003007","","300*300防滑地砖楼面","1.水泥浆一道（内掺建筑胶）\n2.M15水泥防水砂浆（掺3%防水剂）做找坡坡向地漏，最薄处≥20mm厚，上翻墙面不小于250mm、四周延伸不小于500mm\n3.JS防水涂料（清单另列）\n4.20厚M20水泥砂浆\n5.防滑地砖300*300，勾缝\n6.其余满足设计要求","m2","1533.41","55.83"]
["51","011102001003","","花岗石坡道及地面","1.素土夯实\n2.100mm厚碎砖（石、卵石）垫层，宽出面层100mm\n3.80mm厚C15砼\n4.素水泥浆一道（内掺建筑胶）\n5.30mm厚1:3干硬性水泥砂浆粘结层\n6.撒素水面(洒适量清水)\n7.30mm厚花岗石面层，表面斩毛或机刨\n8.具体做法详见设计说明","m2","37.2","66.63"]
["52","011107004003","","水泥豆石台阶面","1.水泥浆一道（内掺建筑胶）\n2.30厚M20水泥豆石面层铁板赶光\n3.其余满足设计要求\n","m2","1.68","28.96"]
["53","011106004003","","水泥砂浆楼梯","1.水泥浆一道（内掺建筑胶）\n2.20mm厚M15水泥砂浆找平压光\n3.其余满足设计要求\n","m2","270.5","31.64"]
["54","011105003004","","块料踢脚线","1.基层处理\n2.10mm厚M20水泥砂浆找平层，分两次压实抹平\n3.专用胶粘结层\n4.10mm厚地砖踢脚，勾缝\n5.其余满足设计要求及相关规范","m2","143","123.25"]
["55","011101003006","","细石混凝土楼地面 楼6","1.水泥浆一道（内掺建筑胶）\n2.20mm厚M20水泥砂浆找平层（清单另列）\n3.9mm厚聚乙烯隔声保温复合卷材（燃烧性能B1级）（清单另列）\n4.30mm厚C20细石砼，双向φ1.2@150钢丝网\n5.其余满足设计要求","m2","7860.65","15.22"]
["56","011103004003","","隔声保温复合卷材楼地面","1.9mm厚聚乙烯隔声保温复合卷材（燃烧性能B1级）","m2","7860.65","29.86"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0109 屋面及防水工程 ",""," "," "," "]
["57","010514002003","","成品水簸箕","1.成品水簸箕C20\n2.其他详见设计","个","2","66.48"]
["58","010902003009","","上人平屋面 屋面1","1.水泥炉渣2%找坡，最薄处30mm厚（清单另列）\n2.20mm厚M15水泥砂浆找平层\n3.2mm厚JS防水涂料（清单另列）\n4.防水卷材（清单另列）\n5.防水卷材（清单另列）\n6.干铺200g/㎡聚酯无纺布\n7.保温板(清单另列)\n8.15mm厚M15水泥砂浆找平层\n9.40mm厚C20细石刚性保护层，内配筋φ6@200×200mm钢筋网单层双向,分割缝间距距3m*3m，宽深20mm，内嵌填聚乙烯泡沫棒、面嵌填建筑密封胶\n10.具体做法详见设计图\n11.其他：满足设计及规范要求","m2","484.64","40.95"]
["59","010902003010","","非上人平屋面 屋面2","1.水泥炉渣2%找坡，最薄处30mm厚（清单另列）\n2.20mm厚M15水泥砂浆找平层\n3.2mm厚JS防水涂料（清单另列）\n4.防水卷材（清单另列）\n5.防水卷材（清单另列）\n6.20mm厚M15水泥砂浆，设间距不大于1*1m分仓缝，缝宽20mm、油膏嵌缝\n7.具体做法详见设计图\n8.其他：满足设计及规范要求","m2","123.25","23.87"]
["60","010901001003","","瓦屋面 屋面3","1.15mm厚M15水泥砂浆找平层\n2.2mm厚JS防水涂料（清单另列）\n3.防水卷材（清单另列）\n4.15mm厚M15水泥砂浆找平层\n5.40mm厚C20细石刚性保护层，内配筋φ6@200×200mm钢筋网单层双向\n6.顺水条40*20\n7.挂瓦条30*30\n8.水泥瓦（固定于挂瓦条上）\n9.具体做法详见设计图\n10.其他：满足设计及规范要求","m2","447.15","19.44"]
["61","010902003011","","外露板顶面","1.水泥浆一道（内掺建筑胶）\n2.M20水泥防水砂浆坡向地漏或出水口，最薄处≥20mm厚\n3.JS防水涂料（清单另列）\n4.20厚M20水泥砂浆\n5.其余满足设计要求","m2","50.31","23.87"]
["62","010902003012","","种植屋面 屋面4","1.水泥炉渣2%找坡，最薄处30mm厚（清单另列）\n2.20mm厚M15水泥砂浆找平层\n3.2mm厚JS防水涂料（清单另列）\n4.防水卷材（清单另列）\n5.防水卷材（清单另列）\n6.干铺200g/㎡聚酯无纺布\n7.保温板(清单另列)\n8.15mm厚M15水泥砂浆找平层\n9.40mm厚C20细石刚性保护层\n10.20mm高凹凸型排（蓄）水板\n11.无纺布过滤层（质量不小于200g/㎡）\n12.300mm厚种植土\n13.植被层（业主自理）\n14.具体做法详见设计图\n15.其他：满足设计及规范要求","m2","244.61","43.64"]
["63","010902008002","","屋面变形缝","1.坡屋面变形缝详西南18J202-4/38\n2.其他做法详见设计大样图","m","7.3","75.52"]
["64","010903001003","","对外门窗洞口用聚合物水泥砂浆加耐碱纤维网布增强层","1.对外门窗洞口应用聚合物水泥砂浆加耐碱纤维网布增强层\n2.具体做法详见设计图","m2","936.12","18.79"]
["65","010903004002","","外墙变形缝","1.做法详见西南18J516-1/69","m","100.9","51.86"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0110 保温、隔热、防腐工程 ",""," "," "," "]
["66","011001001007","","屋面水泥炉渣找坡层","1.1:6水泥炉渣找坡\n2.具体做法详见设计图\n3.其他：满足设计及施工验收规范要求","m3","77.89","185.98"]
["67","011001001009","","卫生间水泥炉渣回填","1.回填材料：1:6沥青炉渣回填\n2.其它：满足设计及相关规范要求","m3","201.12","184.23"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0112 墙、柱面装饰与隔断、幕墙工程 ",""," "," "," "]
["68","011201001009","","内墙面一般抹灰 架空层内1","1.基层处理\n2.20mm厚M15水泥石灰膏砂浆分遍抹平\n3.柔性耐水腻子(清单另列）\n4.其余满足设计要求及相关规范\n","m2","293.57","24.12"]
["69","011201001010","","内墙面一般抹灰 内1+内2","1.基层处理\n2.20mm厚M15水泥石灰砂浆分遍抹平\n3.其余满足设计要求及相关规范","m2","28182","25.81"]
["70","011204003004","","面砖内墙面 内3","1.基层处理、10mm厚M20水泥砂浆找平层，分两次压实抹平(清单另列)\n2.防水层（清单另列）\n3.20mm厚M20水泥砂浆\n4.专用胶粘结层\n5.300*600墙面砖（规格详内装设计，综合考虑），勾缝\n6.其他：满足设计、施工及验收规范要求","m2","6116.25","53.36"]
["71","011201001011","","外墙面一般抹灰","1.基层处理\n2.20mm厚M15水泥砂浆找平层（掺5%CH-B防水剂）；\n","m2","16192.37","34.47"]
["72","011201001012","","女儿墙内侧墙面一般抹灰","1.基层处理\n2.20mm厚M15水泥砂浆找平层（掺5%CH-B防水剂）；\n3.其余满足设计要求及相关规范\n","m2","1757.92","25.73"]
["73","011201004008","","内墙面水泥砂浆找平层 内3","1.基层处理\n2.20mm厚M20水泥砂浆找平层，分两次压实抹平\n3.其余满足设计要求及相关规范","m2","7536.29","16.34"]
["74","011201004009","","内墙面水泥砂浆找平层 内4","1.基层处理\n2.20mm厚M20水泥砂浆找平层，分两次压实抹平\n3.其余满足设计要求及相关规范","m2","2537.92","15.79"]
["75","011201004010","","外墙面变形缝内墙面找平","1.基层处理\n2.20mm厚M10水泥砂浆（掺5%CH-B防水剂）\n3.其余满足设计要求及相关规范","m2","552.32","13.61"]
["76","011201004011","","内墙面找平","1.基层处理\n2.20mm厚M10水泥砂浆\n3.其余满足设计要求及相关规范","m2","2019.8","13.61"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0113 天棚工程 ",""," "," "," "]
["77","011302001003","","防潮石膏板吊顶 顶1","1.基层清理\n2.配套轻钢龙骨（参西南18J515-68-P9)\n3.12mm厚防潮石膏板（设检修口） \n4.2mm厚腻子分遍磨平、刷无机涂料\n5.其余满足设计要求及相关规范\n","m2","1241.84","66.24"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0114 油漆、涂料、裱糊工程 ",""," "," "," "]
["78","011406003007","","百叶内墙面及天棚面满刮腻子","1.基层清理\n2.刮外墙专用柔性耐水腻子两遍","m2","2069.14","9.82"]
["79","011406001007","","飘窗地面乳胶漆","1.刷水泥浆一道（内掺建筑胶）\n2.腻子种类：2mm厚柔性耐水腻子\n3.乳胶漆饰面，一底两面","m2","456.63","19.30"]
["80","011406001008","","室内墙面乳胶漆","1.刷水泥浆一道（内掺建筑胶）\n2.腻子种类：2mm厚柔性耐水腻子\n3.乳胶漆饰面，一底两面","m2","26635.48","19.30"]
["81","011407002005","","悬挑板底面喷刷涂料","1.基层清理\n2.素水泥浆一道甩毛（内掺建筑胶）\n3.2mm厚柔性腻子分遍刮平\n4.无机涂料，一底两面（外墙）\n5.包含独立梁面，其余满足设计要求及相关规范","m2","456.63","28.39"]
["82","011406001009","","外墙真石漆涂料","1.刮外墙专用柔性耐水腻子两遍\n2.涂刷防潮抗碱封闭底漆\n3.喷真石漆涂料两遍\n4.喷甲基硅醇钠憎水剂\n5.分格及具体做法详见设计大样图","m2","15868.6","26.91"]
["83","011406003008","","内墙满刮腻子 ","1.基层类型：综合\n2.腻子种类：2mm厚柔性耐水腻子\n3.刮腻子遍数：满刮腻子、砂磨平","m2","293.57","9.94"]
["84","011406003009","","天棚耐水腻子","1.腻子种类：2mm厚柔性耐水腻子\n2.刮腻子遍数：满刮腻子、砂磨平","m2","237.08","9.94"]
["85","011407001003","","内墙无机涂料","1.2mm厚柔性耐水腻子分遍刮平\n2.无机涂料，一底两面（深色踢脚综合考虑报价，不单独列项）\n3.包含独立柱面，其余满足设计要求及相关规范","m2","1546.52","18.38"]
["86","011407002006","","天棚喷刷涂料","1.2mm厚柔性耐水腻子分遍刮平\n2.无机涂料，一底两面\n3.包含独立梁面，其余满足设计要求及相关规范","m2","11304.34","24.81"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0115 其他装饰工程 ",""," "," "," "]
["87","011501018003","","成品信报箱","1.台柜规格：成品信报箱\n2.详设计","个","2","3089.13"]
["88","011503002005","","楼梯栏杆 H=900mm","1..栏杆材料种类、规格、品牌：详见西南18J412-47-5\n2.固定配件种类：满足设计规范及要求\n3.栏杆高度：0.9m\n4.除锈、油漆、预埋件、螺栓固定件等内容的费用包含在综合单价中\n5.其他：满足设计、施工及验收规范要求","m","165.78","73.60"]
["89","011503002006","","楼梯栏杆 H=1000mm","1..栏杆材料种类、规格、品牌：详见西南18J412-47-5\n2.固定配件种类：满足设计规范及要求\n3.栏杆高度：净高1.0m\n4.除锈、油漆、预埋件、螺栓固定件等内容的费用包含在综合单价中\n5.其他：满足设计、施工及验收规范要求","m","2.6","73.60"]
["90","011503001005","","护窗栏杆 H=900mm","1.横杆材料种类、规格：□50*60*1.5铁矩管、40*40*1.5铁矩管\n2.立柱材料种类、规格：□50*50*2.5铁矩管\n3.竖杆材料种类、规格：□25*25*1.5铁矩管\n4.预埋及其它埋置方式由投标人自行考虑在投标报价中，结算不作调整\n5.做法参西南18J412-61-2B，具体做法详见设计大样图\n6.刷漆：满足设计及规范要求","m","950","73.60"]
["91","011503001006","","护窗栏杆 H=1100mm","1.横杆材料种类、规格：□50*60*1.5铁矩管、40*40*1.5铁矩管\n2.立柱材料种类、规格：□50*50*2.5铁矩管\n3.竖杆材料种类、规格：□25*25*1.5铁矩管\n4.预埋及其它埋置方式由投标人自行考虑在投标报价中，结算不作调整\n5.做法参西南18J412-61-2B，具体做法详见设计大样图\n6.刷漆：满足设计及规范要求","m","21.4","73.60"]
["92","011503005003","","楼梯间靠墙扶手","1.扶手材料种类、规格、品牌：Φ50钢管扶手\n2.预埋及其它埋置方式由投标人自行考虑在投标报价中，结算不作调整\n3.刷漆：满足设计及规范要求","m","5.7","35.89"]
["93","011503008003","","玻璃栏板 H=1100mm","1.扶手材料种类、规格、品牌：φ50*3钢管扶手\n2.立杆材料种类、规格、品牌：φ60*3钢管\n3.玻璃种类、规格：8+1.52PVB+8mm钢化夹胶玻璃\n4.安装方式应根据设计做法予以考虑，结算不作调整\n5.预埋及其它埋置方式由投标人自行考虑在投标报价中，结算不作调整\n6.刷漆：满足设计及规范要求","m","1109.8","76.61"]
["94","011502001003","","铝合金格栅","1.铝合金格栅50*50*1.2\n2.具体做法详见设计图纸","m","612","47.67"]
["95","011501009003","","厨房灶台","1.厨房灶台","个","188","24.48"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","单价措施项目清单 ",""," "," "," "]
[" "," ","","脚手架工程 ",""," "," "," "]
["96","011701001003","","综合脚手架","1.搭设方式：投标人自行考虑报价，施工中无论采用何种搭设方式，结算均不作调整\n2.搭设高度：投标人自行考虑报价 \n3.脚手架材质：投标人自行考虑报价，施工中无论采用何种材质，结算均不作调整\n4.本清单工程量包含不同檐高的裙房的建筑面积，其费用在本项综合单价中综合考虑\n5.需单独计算的外脚手，工程量另列清单\n6.其他：满足设计、施工及验收规范要求","m2","14704.55","13.37"]
["97","011701002003","","外脚手架","1.搭设方式 ：钢管架、提升架、外装饰吊篮等综合考虑。\n2.搭设高度 ：投标人自行考虑。\n3.脚手架材质由投标人根据工程实际情况按照国家现行标准规范自行确定，结算时不因搭设方式的不同而调整。\n4.其它：满足施工图设计要求及施工验收规范要求。","m2","16693.38","19.15"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","混凝土模板及支架（撑 ） ",""," "," "," "]
["98","011702001003","","垫层模板安拆","1.使用部位：垫层\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","24.92","36.84"]
["99","011702002005","","矩形柱模板安拆","1.使用部位：矩形柱\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.超高增加费另计\n5.其他：满足设计、施工及验收规范要求","m2","74.9","59.84"]
["100","011702002006","","矩形柱模板每超高1m增加费","1.矩形柱模板每超高1m增加费","m2","149.8","5.08"]
["101","011702011007","","屋面挡墙模板安拆","1.使用部位：屋面挡墙模板安拆\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.其他：满足设计、施工及验收规范要求","m2","170.99","59.14"]
["102","011702011008","","直形墙模板安拆","1.使用部位：直形墙，包含剪力墙中的暗柱、暗梁\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.超高增加费另计\n5.其他：满足设计、施工及验收规范要求","m2","26852.32","65.06"]
["103","011702011009","","直形墙模板每超高1m增加费","1.直形墙模板每超高1m增加费","m2","1295.92","4.95"]
["104","011702014005","","有梁板模板安拆","1.使用部位：有梁板模板安拆\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.超高增加费另计\n5.钢筋砼板底面清理干净、找平层包含在单价内\n6.其他：满足设计、施工及验收规范要求","m2","20329.91","60.26"]
["105","011702014006","","管井后浇板模板安拆","1.使用部位：管井后浇板\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.超高增加费另计\n5.其他：满足设计、施工及验收规范要求","m2","141.8","60.26"]
["106","011702003003","","构造柱模板安拆","1.使用部位：构造柱综合考虑\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","3750.95","55.63"]
["107","011702006005","","矩形梁模板安拆","1.构件类型：除有梁板以外的矩形梁\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","106.74","57.29"]
["108","011702006006","","矩形梁模板每超高1m增加费","1.构件类型：除有梁板以外的矩形梁\n","m2","167.55","6.08"]
["109","011702009003","","过梁模板安拆","1.构件类型：过梁\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","508.42","67.43"]
["110","011702021003","","凸窗侧墙板模板安拆","1.构件类型：栏板\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","1888.32","66.31"]
["111","011702023003","","悬挑板模板安拆","1.构件类型：综合考虑悬挑板、凸窗板、雨棚板\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","2064.65","72.58"]
["112","011702008005","","圈梁模板安拆","1.使用部位：圈梁及现浇带\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","125.77","57.72"]
["113","011702024003","","楼梯模板安拆","1.使用部位：楼梯\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","270.5","135.69"]
["114","011702016003","","平板模板安拆","1.使用部位：平板模板安拆\n2.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n3.支架材料：钢管、竹、木支架等综合\n4.超高增加费另计\n5.其他：满足设计、施工及验收规范要求","m2","16.23","56.41"]
["115","011702028003","","压顶模板安拆","1.使用部位：压顶\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","49.56","53.68"]
["116","011702025005","","其它构件模板安拆","1.使用部位：屋面踏步等零星\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","12.4","78.96"]
["117","011702025006","","边框模板安拆","1.使用部位：根据图集构造要求，洞口宽度仅>1.8m且≤2.1m时设置\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","63.36","77.79"]
["118","011702029003","","散水模板安拆","1.使用部位：散水\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","7.48","36.84"]
["119","011702008006","","翻边、挡水及门槛模板安拆","1.构件类型：翻边、挡水及门槛\n2.支模高度：各种高度综合\n3.模板类型：复合模板、木模、组合钢模板、竹胶板等综合\n4.支架材料：钢管、竹、木支架等综合\n5.其他：满足设计、施工及验收规范要求","m2","732.45","57.72"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","垂直运输 ",""," "," "," "]
["120","011703001003","","垂直运输","1.建筑物建筑类型及结构形式：详设计\n2.建筑物檐口高度：详设计\n3.本清单工程量包含不同檐高的裙房的建筑面积，其费用在本项综合单价中综合考虑","m2","14704.55","17.34"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","超高施工增加 ",""," "," "," "]
["121","011704001003","","超高施工增加","1.建筑物建筑类型及结构形式：详设计,综合考虑\n2.建筑物檐口高度、层数：详设计,综合考虑\n3.单层建筑物檐口高度超过20m，多层建筑物超过6层部分的建筑面积","m2","8956.72","28.17"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","分部小计 ",""," "," "," "]
["合    计","","","","","","",""]

{"sheet":"K.2 承包人提供主要材料和工程设备一览表(表-20)【B-~","index":4,"n_rows":42,"n_cols":12,"rows_kept":42,"merged":[[0,0,0,11],[1,1,1,6],[1,7,1,9],[1,10,1,11],[2,1,2,3],[2,6,2,7],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2]],"flags":["formulas_cached_only"]}
[" 承包人提供主要材料和工程设备一览表\r\n（适用造价信息差额调整法）",null,null,"","","","","","","","",""]
["工程名称：","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【建筑与装饰工程】",{"$nulls":5},"标段：/",null,null,""]
["序号","名称、规格、型号",null,null,"单位","数量","风险系数%",null,"基准单价(元)","招标控制单价(元)","发承包人确认单价(元)","备注"]
["14","XY401粘接剂",null," ","kg","2358.21",{"$nulls":3},"12.10"]
["15","白水泥",null," ","kg","8210.18",{"$nulls":3},"0.61"]
["16","板枋材",null," ","m3","0.107",{"$nulls":3},"2065.42"]
["23","不锈钢六角螺栓带螺母",null,"M6×50以下","10套","388.208",{"$nulls":3},"20.66"]
["24","柴油(机械)",null," ","L","6009.628",{"$nulls":3},"7.29"]
["27","成品信报箱",null," ","个","2",{"$nulls":3},"3064.65"]
["30","低合金钢焊条",null,"E43系列","kg","72.268",{"$nulls":3},"8.58"]
["31","电焊丝",null," ","kg","11.412",{"$nulls":3},"5.04"]
["34","镀锌螺钉",null,"带垫","个","2875.444",{"$nulls":3},"0.05"]
["35","对拉螺栓",null," ","kg","5891.526",{"$nulls":3},"5.04"]
["36","对拉螺栓塑料管",null," ","m","38724.44",{"$nulls":3},"1.33"]
["44","二等锯材",null," ","m3","390.25",{"$nulls":3},"2065.42"]
["45","二甲苯",null," ","kg","1493.533",{"$nulls":3},"9.11"]
["46","复合模板",null," ","m2","15054.618",{"$nulls":3},"25.21"]
["57","焊条",null,"综合","kg","2665.271",{"$nulls":3},"5.04"]
["58","合金钢钻头",null,"综合","个","434.184",{"$nulls":3},"10.08"]
["64","加工铁件",null," ","kg","341.54",{"$nulls":3},"5.04"]
["67","脚手架钢材",null," ","kg","12765.869",{"$nulls":3},"5.04"]
["69","锯材",null,"综合","m3","34.24",{"$nulls":3},"2065.42"]
["75","梁柱节点金属网",null," ","m2","64.975",{"$nulls":3},"1.35"]
["93","其他材料费",null," ","元","207550.501",{"$nulls":3},"1.22"]
["94","汽油",null," ","L","2722.755",{"$nulls":3},"7.90"]
["100","软蜡",null," ","kg","180.796",{"$nulls":3},"11.09"]
["102","杉原木",null,"综合","m3","7.922",{"$nulls":3},"1336.45"]
["118","水",null," ","m3","6420.401",{"$nulls":3},"3.40"]
["126","摊销卡具和支撑钢材",null," ","kg","23973.762",{"$nulls":3},"5.04"]
["128","铁件",null," ","kg","1051.682",{"$nulls":3},"5.04"]
["129","铜丝",null," ","kg","24.512",{"$nulls":3},"23.19"]
["152","植筋胶泥",null," ","kg","382.747",{"$nulls":3},"15.12"]
["154","棕垫",null," ","kg","9.792",{"$nulls":3},"5.04"]
[3,"10mm厚地砖踢脚",null," ","m2","145.86",{"$nulls":3},"31.85"]
["26","成品水簸箕",null," ","个","2",{"$nulls":3},"42.00"]
["83","铝合金格栅",null," ","m2","642.6",{"$nulls":3},"42.01"]
["85","麻刀",null," ","kg","5651.713",{"$nulls":3},"4.03"]
["95","砌块墙钢丝网加固",null," ","m2","9928.065",{"$nulls":3},"1.35"]
["117","双面胶纸带",null," ","m2","1152.378",{"$nulls":3},"20.17"]
["130","屋面钢楼梯",null," ","t","3.6",{"$nulls":3},"6874.48"]
["131","屋面检修梯",null," ","t","0.074",{"$nulls":3},"6940.22"]
["145","预埋铁件",null," ","kg","620.967",{"$nulls":3},"5.04"]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)~1","index":5,"n_rows":109,"n_cols":12,"rows_kept":109,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[65,1,65,2],[66,1,66,2],[67,1,67,2],[68,1,68,2],[69,1,69,2],[70,1,70,2],[71,1,71,2],[71,3,71,4],[72,1,72,2],[72,3,72,4],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[82,3,82,4],[83,1,83,2],[83,3,83,4],[84,1,84,2],[84,3,84,4],[85,1,85,2],[86,1,86,2],[86,3,86,4],[87,1,87,2],[87,3,87,4],[88,1,88,2],[89,1,89,2],[90,1,90,2],[91,1,91,2],[92,1,92,2],[93,1,93,2],[94,1,94,2],[95,1,95,2],[96,1,96,2],[97,1,97,2],[98,1,98,2],[99,1,99,2],[100,1,100,2],[101,1,101,2],[102,1,102,2],[103,1,103,2],[104,1,104,2],[105,1,105,2],[106,1,106,2],[106,3,106,4],[107,1,107,2],[107,3,107,4],[108,0,108,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【强电工程】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","电气设备安装工程 ",""," "," "," "," "," "," "," "]
["1","030404017027","","住宅转接箱 ALMZ-1","1.名称：住宅转接箱 ALMZ-1\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["2","030404017028","","住宅转接箱 ALMZ-2","1.名称：住宅转接箱 ALMZ-2\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["3","030404017029","","住宅转接箱 ALMZ-3","1.名称：住宅转接箱 ALMZ-3\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["4","030404017030","","住宅电表箱 AW-1","1.名称：住宅电表箱 AW-1\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["5","030404017031","","住宅电表箱 AW-2","1.名称：住宅电表箱 AW-2\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","14","456.35"]
["6","030404017032","","家居配电箱 ALH-B6","1.名称：家居配电箱 ALH-B6\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","188","128.37"]
["7","030404017033","","应急照明配电箱 ALE","1.名称：应急照明配电箱 ALE\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["8","030404017034","","应急照明配电箱 3、9、15ALE","1.名称：应急照明配电箱 3、9、15ALE\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","6","456.35"]
["9","030404017035","","消防动力配电箱 B1AP-ZXF*、B1APE-ZXF*","1.名称：消防动力配电箱 B1AP-ZXF*、B1APE-ZXF*\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","4","456.35"]
["10","030404017036","","照明配电箱 4AL1","1.名称：照明配电箱 4AL1\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["11","030404017037","","照明配电箱 13AL1","1.名称：照明配电箱 13AL1\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["12","030404017038","","消防电梯配电箱 D-AT-XT","1.名称：消防电梯配电箱 D-AT-XT\n2.型号：各种类型配电箱、控制箱、箱体尺寸综合考虑\n3.规格：详设计\n4.安装方式:综合考虑，满足设计及规范要求\n5.本项目包括开箱、检查、安装、箱柜开孔、防火封堵、进出箱的压接线及盘柜二次配线、本体接地、补刷油漆、标识等\n6.不含消防电源监控模块、电压信号传感器、电气火灾探测器、RS485接口及其管线 \n7.为完成本项目安装的所有工作内容,其余满足设计、施工及供电验收等规范要求等费用综合考虑进入本项目综合单价中。\n8.其他：满足设计及规范要求","台","2","456.35"]
["13","030408001014","","预分支电缆 WDZR-YFD-YJY-4(1*70)+1(1*35)mm2","1.名称：预分支电缆 \n2.规格型号 ：WDZR-YFD-YJY-4(1*70)+1(1*35)mm2\n3.材质：铜芯\n4.敷设方式、部位：电缆托盘、穿管、井道内等综合考虑\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","80","8.04"]
["14","030408001015","","预分支电缆 WDZR-YFD-YJY-4(1*185)+1(1*95)mm2","1.名称：预分支电缆 \n2.规格型号 ：WDZR-YFD-YJY-4(1*185)+1(1*95)mm2\n3.材质：铜芯\n4.敷设方式、部位：电缆托盘、穿管、井道内等综合考虑\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","82.8","8.04"]
["15","030408001016","","矿物绝缘电缆 NG-A-5*4mm2","1.名称：矿物绝缘电缆\n2.规格、型号：NG-A-5*4mm2\n3.材质：铜芯\n4.敷设方式、部位：桥架、管内\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","52","8.04"]
["16","030408001017","","矿物绝缘电缆 NG-A-4*25+1*16mm2","1.名称：矿物绝缘电缆\n2.规格、型号：NG-A-4*25+1*16mm2\n3.材质：铜芯\n4.敷设方式、部位：桥架、管内\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","250.82","8.04"]
["17","030408006014","","预分支电缆头 WDZR-YFD-YJY-4(1*70)+1(1*35)mm2","1.名称：预分支电缆头\n2.规格、型号：WDZR-YFD-YJY-4(1*70)+1(1*35)mm2\n3.材质、类型：综合考虑  \n4.安装部位：室内\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","个","16","54.79"]
["18","030408006015","","预分支电缆头 WDZR-YFD-YJY-4(1*185)+1(1*95)mm2","1.名称：预分支电缆头\n2.规格、型号：WDZR-YFD-YJY-4(1*185)+1(1*95)mm2\n3.材质、类型：综合考虑  \n4.安装部位：室内\n5.电压等级（kV）：0.6/1kV\n6.其他要求：满足设计、相关图集、标准及招标技术要求","个","6","54.79"]
["19","030408006016","","矿物电缆头 五芯 截面 ≤10mm2","1.名称：矿物电缆电缆头  \n2.型号：综合  \n3.规格：五芯 截面≤10mm2 \n4.材质、类型 ：综合考虑 \n5.其他：满足设计及规范要求","个","8","54.79"]
["20","030408006017","","矿物电缆头 五芯 截面 ≤35mm2","1.名称：矿物电缆电缆头  \n2.型号：综合  \n3.规格：五芯 截面≤35mm2 \n4.材质、类型 ：综合考虑 \n5.其他：满足设计及规范要求","个","8","54.79"]
["21","030411004031","","电气配线 BV-2.5mm2","1.名称:电气配线 \n2.配线形式:管内穿线、线槽配线综合 \n3.型号、规格:BV-2.5mm2\n4.材质:铜\n5.本项目双色线价差考虑在综合单价内\n6.其他：满足设计及相关规范要求","m","21414.35","1.39"]
["22","030411004032","","电气配线 BV-4mm2","1.名称:电气配线 \n2.配线形式:管内穿线、线槽配线综合 \n3.型号、规格:BV-4mm2\n4.材质:铜\n5.本项目双色线价差考虑在综合单价内\n6.其他：满足设计及相关规范要求","m","67872.82","1.39"]
["23","030411004033","","电气配线 WDZN-BYJ-2.5mm2","1.名称:电气配线 \n2.配线形式:管内穿线、线槽配线综合 \n3.型号、规格:WDZN-BYJ-2.5mm2\n4.材质:铜\n5.本项目双色线价差考虑在综合单价内\n6.其他：满足设计及相关规范要求","m","3966.8","1.39"]
["24","030411004034","","电气配线 WDZN-BYJ-4mm2","1.名称:电气配线 \n2.配线形式:管内穿线、线槽配线综合 \n3.型号、规格:WDZN-BYJ-4mm2\n4.材质:铜\n5.本项目双色线价差考虑在综合单价内\n6.其他：满足设计及相关规范要求","m","549","1.39"]
["25","030411004035","","电气配线 WDZ-BYJ-16mm2","1.名称:电气配线 \n2.配线形式:管内穿线、线槽配线综合 \n3.型号、规格:WDZ-BYJ-16mm2\n4.材质:铜\n5.本项目双色线价差考虑在综合单价内\n6.其他：满足设计及相关规范要求","m","9733.99","1.39"]
["26","030411001042","","电气配管 JDG20","1.名称：电气穿线管\n2.材质：JDG\n3.规格：JDG20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","46.31","5.70"]
["27","030411001043","","电气配管 JDG32","1.名称：电气穿线管\n2.材质：JDG\n3.规格：JDG32\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","909.05","5.70"]
["28","030411001044","","电气配管 SC20","1.名称：电气穿线管\n2.材质：镀锌钢管\n3.规格：SC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","1635.7","5.70"]
["29","030411001045","","电气配管 SC32","1.名称：电气穿线管\n2.材质：镀锌钢管\n3.规格：SC32\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","40","5.70"]
["30","030411001046","","电气配管 SC65","1.名称：电气穿线管\n2.材质：镀锌钢管\n3.规格：SC65\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","10","5.70"]
["31","030411001047","","电气配管 PC20","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","7864","6.94"]
["32","030411001048","","电气配管 PC25","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC25\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","21977.14","5.70"]
["33","030411003013","","强电梯架（电井敷设） 300*100","1.名称：强电梯架（电井敷设）\n2.型号、规格：300*100\n3.材质：钢质(厚度符合规范要求)\n4.类型：含隔板、盖板、扣锁、弯通、三通、四通、连接片螺栓等各种配件\n5.接地方式：电气竖井内敷设的电缆桥架或金属线槽应不少于两处与接地干线相连接\n6.桥架含连接穿线管时线槽开孔、过伸缩缝、沉降缝处理等内容\n7.桥架内接地扁钢25*4以及桥架支架另计\n8.其他要求：满足设计、相关图集、标准及招标技术要求","m","97","19.27"]
["34","030411003014","","消防强电线槽（电井敷设） NH-MR-150*100","1.名称：消防强电线槽（电井敷设）\n2.型号、规格：NH-MR-150*100\n3.材质：钢质(厚度符合规范要求)\n4.类型：含隔板、盖板、扣锁、弯通、三通、四通、连接片螺栓等各种配件\n5.接地方式：电气竖井内敷设的电缆桥架或金属线槽应不少于两处与接地干线相连接\n6.桥架含连接穿线管时线槽开孔、过伸缩缝、沉降缝处理等内容\n7.桥架内接地扁钢25*4以及桥架支架另计\n8.其他要求：满足设计、相关图集、标准及招标技术要求","m","97","19.27"]
["35","030411003015","","强电线槽 MR-150*75","1.名称：强电线槽\n2.型号、规格：MR-150*75\n3.材质：钢质(厚度符合规范要求)\n4.类型：含隔板、盖板、扣锁、弯通、三通、四通、连接片螺栓等各种配件\n5.接地方式：电气竖井内敷设的电缆桥架或金属线槽应不少于两处与接地干线相连接\n6.桥架含连接穿线管时线槽开孔、过伸缩缝、沉降缝处理等内容\n7.桥架内接地扁钢25*4以及桥架支架另计\n8.其他要求：满足设计、相关图集、标准及招标技术要求","m","678.38","19.27"]
["36","030409002011","","桥架内接地线 热镀锌扁钢 -25*4","1.名称：户内接地母线\n2.材质：热镀锌扁钢 \n3.型号规格：-25*4\n4.其他：满足设计及规范要求","m","872.38","14.53"]
["37","030408008005","","防火堵料","1.名称：防火堵料\n2.材质：井道内、桥架穿墙、保护管封堵等综合考虑\n3.方式：满足设计及规范要求\n4.部位：综合考虑\n5.其他：满足设计及规范要求","t","0.224","7347.78"]
["38","030413001005","","桥架支、吊架制作安装","1.名称:桥架支架制作、安装\n2.材质:型钢\n3.规格:综合\n4.刷油防腐符合规范和设计要求\n5.其他要求：满足设计、相关图集、标准及招标技术要求","kg","885.17","7.82"]
["39","030404033003","","换气扇","1.名称：换气扇 \n2.型号、规格：详设计 \n3.安装方式：综合考虑","台","2","91.47"]
["40","030412001015","","单管应急荧光壁灯(带防火罩)","1.名称:单管应急荧光壁灯(带防火罩)\n2.规格、型号:220V LED 1*18W \n3.安装方式：综合考虑\n4.其他：满足设计及规范要求","套","4","26.36"]
["41","030412004009","","安全出口标志灯","1.名称：安全出口标志灯\n2.型号：36V LED 2W \n3.安装形式:门框上方0.2m挂装\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他：满足设计、规范及招标技术要求","套","4","31.30"]
["42","030412004010","","疏散出口标志灯","1.名称：疏散出口标志灯\n2.型号：36V LED 2W \n3.安装形式:门框上方0.2m挂装\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他：满足设计、规范及招标技术要求","套","64","31.30"]
["43","030412004011","","方向疏散标志灯具","1.名称：方向疏散标志灯具\n2.型号：36V LED 2W \n3.安装形式:挂壁底边距地0.5米\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他：满足设计、规范及招标技术要求","套","66","31.30"]
["44","030412004012","","楼层指示灯","1.名称:楼层指示灯\n2.型号：36V LED 2W \n3.安装形式:底边距地2.4m挂装\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他：满足设计、规范及招标技术要求","套","34","31.30"]
["45","030412001016","","应急照明灯","1.名称：应急照明灯\n2.规格、型号：36V LED 5W \n3.安装形式：底边距地2.5m\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他要求：满足设计、相关图集、标准及招标技术要求","套","4","31.30"]
["46","030412005003","","附微波感应灯","1.名称：附微波感应灯\n2.规格、型号：平时感应点亮时12W、1200lm,节电模式时30lm;应急点亮时4W、400lm\n3.安装形式：吸顶安装\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他要求：满足设计、相关图集、标准及招标技术要求","套","264","31.30"]
["47","030412001017","","防水壁灯","1.名称:防水壁灯\n2.规格、型号:220V  1*13W \n3.安装方式：W,H=2.0m\n4.其他：满足设计及规范要求","套","188","26.36"]
["48","030412001018","","管井专用壁灯","1.名称:管井专用壁灯\n2.规格、型号:220V LED 5W \n3.安装方式：水井内门上口0.2m\n4.其他：满足设计及规范要求","套","64","26.36"]
["49","030412001019","","热释感应灯","1.名称：热释感应灯\n2.规格、型号：220V LED 1*18W \n3.安装形式：吸顶安装\n4.含灯具安装所需光源、灯具附件、焊压接线端子、补刷（喷）油漆、接地等\n5.其他要求：满足设计、相关图集、标准及招标技术要求","套","30","26.36"]
["50","030412001020","","吸顶灯(带灯罩)","1.名称：吸顶灯(带灯罩) \n2.型号、规格：220V  1*18W  \n3.安装形式：吸顶安装\n4.其他要求：满足设计、相关图集、标准及招标技术要求","套","1376","26.36"]
["51","030404035022","","单相二、三极插座","1.名称：单相二、三极插座\n2.型号、规格：250V 10A\n3.安装方式：电井H=1.0m,其他H=0.3m\n4.其他：满足设计、规范及招标技术要求","个","1228","10.88"]
["52","030404035023","","单相二、三极带开关卫生间插座","1.名称：单相二、三极带开关卫生间插座\n2.型号、规格：250V 10A 带防溅盖插座\n3.安装方式：暗装,H=1.50m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["53","030404035024","","单相二、三极电视电源插座","1.名称：单相二、三极电视电源插座\n2.型号、规格：250V 10A\n3.安装方式：暗装,大堂H=0.5m,卧室床头插座H=0.65m\n4.其他：满足设计、规范及招标技术要求","个","752","10.88"]
["54","030404035025","","单相二、三极带开关电炊具插座","1.名称：单相二、三极带开关电炊具插座\n2.型号、规格：250V 10A 带防溅盖插座\n3.安装方式：暗装,厨房H=1.35m\n4.其他：满足设计、规范及招标技术要求","个","440","10.88"]
["55","030404035026","","单相三极抽油烟机插座","1.名称：单相三极抽油烟机插座\n2.型号、规格：250V 10A\n3.安装方式：暗装,H=2.2m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["56","030404035027","","单相三极带开关电冰箱插座","1.名称：单相三极带开关电冰箱插座\n2.型号、规格：250V 10A\n3.安装方式：暗装,厨房H=1.35m,客厅H=0.3m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["57","030404035028","","单相三极带开关高位空调插座","1.名称：单相三极带开关高位空调插座\n2.型号、规格：250V 16A\n3.安装方式：暗装,H=2.2m(底边距地2.2m)\n4.其他：满足设计、规范及招标技术要求","个","378","10.88"]
["58","030404035029","","单相三极低位空调插座","1.名称：单相三极低位空调插座\n2.型号、规格：250V 16A\n3.安装方式：暗装,暗装,H=0.3m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["59","030404035030","","单相三极带开关燃气热水器插座","1.名称：单相三极带开关燃气热水器插座\n2.型号、规格：250V 10A 带防溅盖插座\n3.安装方式：暗装,H=1.60m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["60","030404035031","","单相三极带开关洗衣机插座","1.名称：单相三极带开关洗衣机插座\n2.型号、规格：250V 10A\n3.安装方式：暗装,客厅H=0.6m,大堂H=1.9m,其他H=0.3m\n4.其他：满足设计、规范及招标技术要求","个","188","10.88"]
["61","030404034007","","暗装单联单控开关","1.名称：暗装单联单控开关\n2.型号、规格：220V,10A \n3.安装方式：暗装,户内H=1.3m\n4.其他：满足设计、规范及招标技术要求","个","1064","14.42"]
["62","030404034008","","暗装双联单控开关","1.名称：暗装双联单控开关\n2.型号、规格：220V,10A \n3.安装方式：暗装,户内H=1.3m\n4.其他：满足设计、规范及招标技术要求","个","2","14.42"]
["63","030404034009","","暗装三联单控开关","1.名称：暗装三联单控开关\n2.型号、规格：220V,10A \n3.安装方式：暗装,户内H=1.3m\n4.其他：满足设计、规范及招标技术要求","个","376","14.42"]
["64","030411006017","","接线盒安装（塑料）","1.名称：接线盒安装（塑料）\n2.材质：塑料\n3.规格：86型，含开关、插座、灯头盒等\n4.安装形式：综合考虑\n5.其他要求：满足设计、相关图集、标准及招标技术要求","个","7304","6.03"]
["65","030411006018","","接线盒安装（钢制）","1.名称：接线盒安装（钢制）\n2.材质：钢制\n3.规格：86型，含开关、插座、灯头盒等\n4.安装形式：综合考虑\n5.其他要求：满足设计、相关图集、标准及招标技术要求","个","716","6.03"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","防雷接地 ",""," "," "," "]
["66","030409005005","","避雷网 热镀锌圆钢 Φ10","1.名称：避雷网 \n2.材质：热镀锌圆钢\n3.规格：Φ10\n4.安装形式:女儿墙上避雷带采用明敷\n5.接地跨接\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","488.82","15.06"]
["67","030409005006","","避雷网 热镀锌扁钢 -25*4","1.名称：避雷网 \n2.材质：热镀锌扁钢\n3.规格：-25*4\n4.安装形式:沿屋面暗敷\n5.接地跨接\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","101.53","15.06"]
["68","030409003003","","避雷引下线","1.名称：避雷引下线\n2.引下线：用建筑物所有钢筋混凝土柱子内所有钢筋作引下线,引下线上端与接闪带可靠连接\n3.本次暂按接地电阻测试点上4根主钢筋(＜Φ16)以上主筋通长焊接作为引下线计算\n4.其他要求：满足设计、相关图集、标准及招标技术要求","m","627.14","2.52"]
["69","030409002012","","柱主筋与圈梁钢筋焊接","1.材质：碳钢\n2.规格：综合\n3.安装部位：需要焊接均压环的楼层引下线柱内主筋与圈梁钢筋焊接","处","12","38.69"]
["70","030409008005","","预埋连接板 100*100*6","1.名称：预埋连接板 100*100*6\n2.型号:详设计要求\n3.其他要求：满足设计、相关图集、标准及招标技术要求","台","12","13.34"]
["71","030409008006","","局部等电位箱 SEB","1.名称：局部等电位箱 SEB\n2.型号:详设计要求\n3.其他要求：满足设计、相关图集、标准及招标技术要求","台","222","13.34"]
["72","030409002013","","接地线 热镀锌扁钢 -40*4","1.名称：接地母线\n2.材质：热镀锌扁钢\n3.规格：-40x4\n4.安装部位：室内\n5.安装形式：暗装\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","100.78","14.53"]
["73","030409002014","","接地线 热镀锌扁钢 -25*4","1.名称：接地母线\n2.材质：热镀锌扁钢\n3.规格：-25x4\n4.安装部位：室内\n5.安装形式：暗装\n6.其他要求：满足设计、相关图集、标准及招标技术要求","m","219.44","14.53"]
["74","030414011003","","接地装置调试","1.接地装置调试\n2.调试符合设计文件及GB50150-2016要求\n3.本项调试费用的计取，同时具备并应符合下列条件：（1.有关施工验收规范、标准要求；2.有经过批准的调试方案；3.调试后经有关部门验收。）","系统","1","1203.29"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","单价措施项目清单 ",""," "," "," "]
[" "," ","","其他措施项目 ",""," "," "," "]
["75","031302007017","","高层施工增加费"," ","项","1","27.30"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","专业措施项目 ",""," "," "," "]
["76","031301001017","","吊装加固"," ","项","0"," "]
["77","031301002017","","金属抱杆安装拆除、移位"," ","项","0"," "]
["78","031301003017","","平台铺设、拆除"," ","项","0"," "]
["79","031301004017","","顶升、提升装置"," ","项","0"," "]
["80","031301005017","","大型设备专用机具"," ","项","0"," "]
["81","031301006017","","焊接工艺评定"," ","项","0"," "]
["82","031301007017","","胎（模）具制作、安装、拆除"," ","项","0"," "]
["83","031301008017","","防护棚制作安装拆除"," ","项","0"," "]
["84","031301009017","","特殊地区施工增加"," ","项","0"," "]
["85","031301010017","","安装与生产同时进行施工增加"," ","项","0"," "]
["86","031301011017","","在有害身体健康环境中施工增加"," ","项","0"," "]
["87","031301012017","","工程系统检测、检验"," ","项","0"," "]
["88","031301013017","","设备、管道施工的安全、防冻和焊接保护"," ","项","0"," "]
["89","031301014017","","焦炉烘炉、热态工程"," ","项","0"," "]
["90","031301015017","","管道安拆后的充气保护"," ","项","0"," "]
["91","031301016017","","隧道内施工的通风、供水、供气、供电、照明及通讯设施"," ","项","0"," "]
["92","031301017017","","脚手架搭拆"," ","项","1","294.18"]
["93","031301018017","","其他措施"," ","项","0"," "]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","分部小计 ",""," "," "," "]
["合    计","","","","","","",""]

{"sheet":"K.2 承包人提供主要材料和工程设备一览表(表-20)【B~1","index":6,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,10],[2,0,2,1],[2,5,2,6],[3,0,3,1],[3,5,3,6],[4,0,4,1],[4,5,4,6],[5,0,5,1],[5,5,5,6],[6,0,6,1],[6,5,6,6]],"flags":["formulas_cached_only"]}
[" 承包人提供主要材料和工程设备一览表\r\n（适用造价信息差额调整法）","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【强电工程】","","","","标段：/","","","",""]
["序号","","名称、规格、型号","单位","数量","风险系数%","","基准单价(元)","招标控制单价(元)","发承包人确认单价(元)","备注"]
["1","","脚手架钢材","kg","6.111"," ",""," ","5.04"," "," "]
["2","","锯材 综合","m3","0.011"," ",""," ","2065.42"," "," "]
["3","","其他材料费","元","15.568"," ",""," ","1.22"," "," "]
["4","","柴油(机械)","L","0.763"," ",""," ","7.29"," "," "]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)~2","index":7,"n_rows":56,"n_cols":12,"rows_kept":56,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[17,3,17,4],[18,1,18,2],[18,3,18,4],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[25,3,25,4],[26,1,26,2],[26,3,26,4],[27,1,27,2],[28,1,28,2],[29,1,29,2],[29,3,29,4],[30,1,30,2],[30,3,30,4],[31,1,31,2],[31,3,31,4],[32,1,32,2],[33,1,33,2],[33,3,33,4],[34,1,34,2],[34,3,34,4],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[53,3,53,4],[54,1,54,2],[54,3,54,4],[55,0,55,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【弱电工程】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","0305 综合布线系统 ",""," "," "," "," "," "," "," "]
["1","030411001054","","电气配管 JDG25","1.名称：电气穿线管\n2.材质：JDG\n3.规格：JDG25\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","1765.51","5.70"]
["2","030411001055","","电气配管 PC20","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","5086.75","6.94"]
["3","030411001056","","电气配管 PC25","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC25\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","2894.58","5.70"]
["4","030411001057","","电气配管 PC32","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC32\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","1485.53","8.18"]
["5","030411003016","","弱电线槽 MR-150*75","1.名称：弱电线槽\n2.型号、规格：MR-150*75\n3.材质：钢质(厚度符合规范要求)\n4.类型：含隔板、盖板、扣锁、弯通、三通、四通、连接片螺栓等各种配件\n5.接地方式：电气竖井内敷设的电缆桥架或金属线槽应不少于两处与接地干线相连接\n6.桥架含连接穿线管时线槽开孔、过伸缩缝、沉降缝处理等内容\n7.桥架内接地扁钢25*4以及桥架支架另计\n8.其他要求：满足设计、相关图集、标准及招标技术要求","m","662.82","19.27"]
["6","030411003017","","弱电线槽（电井敷设） MR-200*100","1.名称：弱电线槽（电井敷设）\n2.型号、规格：MR-200*100\n3.材质：钢质(厚度符合规范要求)\n4.类型：含隔板、盖板、扣锁、弯通、三通、四通、连接片螺栓等各种配件\n5.接地方式：电气竖井内敷设的电缆桥架或金属线槽应不少于两处与接地干线相连接\n6.桥架含连接穿线管时线槽开孔、过伸缩缝、沉降缝处理等内容\n7.桥架内接地扁钢25*4以及桥架支架另计\n8.其他要求：满足设计、相关图集、标准及招标技术要求","m","97","19.27"]
["7","030409002015","","桥架内接地线 热镀锌扁钢 -25*4","1.名称：户内接地母线\n2.材质：热镀锌扁钢 \n3.型号规格：-25*4\n4.其他：满足设计及规范要求","m","759.82","14.53"]
["8","030413001006","","桥架支、吊架制作安装","1.名称:桥架支架制作、安装\n2.材质:型钢\n3.规格:综合\n4.刷油防腐符合规范和设计要求\n5.其他要求：满足设计、相关图集、标准及招标技术要求","kg","689.79","7.82"]
["9","030408008006","","防火堵料","1.名称：防火堵料\n2.材质：井道内、桥架穿墙、保护管封堵等综合考虑\n3.方式：满足设计及规范要求\n4.部位：综合考虑\n5.其他：满足设计及规范要求","t","0.224","7347.78"]
["10","030411006022","","接线盒安装（塑料）","1.名称：接线盒安装（塑料）\n2.材质：塑料\n3.规格：86型，含开关、插座、灯头盒等\n4.安装形式：综合考虑\n5.其他要求：满足设计、相关图集、标准及招标技术要求","个","1513","6.03"]
["11","030502003003","","家居配线箱","1.名称:家居配线箱\n2.材质:详设计\n3.规格:综合考虑\n4.安装方式:住户内暗装,H=0.5m\n4.箱内配置详见设计","个","188","92.67"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0305 访客对讲系统 ",""," "," "," "]
["12","030411001058","","电气配管 PC20","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","3377.17","6.94"]
["13","030411001059","","电气配管 PC25","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC25\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","846.43","5.70"]
["14","030411001060","","电气配管 SC20","1.名称：电气穿线管\n2.材质：镀锌钢管\n3.规格：SC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","15.28","5.70"]
["15","030411001061","","电气配管 SC25","1.名称：电气穿线管\n2.材质：镀锌钢管\n3.规格：SC25\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","22.06","5.70"]
["16","030904008036","","安防接线端子箱","1.名称、型号:安防接线端子箱\n2.安装方式:2.2m-W\n3.压铜端子、端子板接线\n4.其他：满足设计及规范要求","台","32","87.31"]
["17","030411006023","","接线盒安装（塑料）","1.名称：接线盒安装（塑料）\n2.材质：塑料\n3.规格：86型，含开关、插座、灯头盒等\n4.安装形式：综合考虑\n5.其他要求：满足设计、相关图集、标准及招标技术要求","个","376","6.03"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","0305 视频监控系统 ",""," "," "," "]
["18","030411001062","","电气配管 PC20","1.名称：电气配管\n2.材质：阻燃型硬塑料管\n3.规格：PC20\n4.配置形式：明配、暗配、吊顶内敷设综合考虑\n5.包含管道除锈刷油、防火处理、接地、防腐处理\n6.其他要求：满足设计、相关图集、标准及招标技术要求\n7.特别说明:含预留孔洞、打孔洞，预留槽、剔槽及混凝土砂浆补孔洞、补槽以及明装敷设管道支架制作、安装，含管件及所有附件；接地（含跨接线），按设计要求刷漆","m","67.62","6.94"]
["19","030411006024","","接线盒安装（塑料）","1.名称：接线盒安装（塑料）\n2.材质：塑料\n3.规格：86型，含开关、插座、灯头盒等\n4.安装形式：综合考虑\n5.其他要求：满足设计、相关图集、标准及招标技术要求","个","8","6.03"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","单价措施项目清单 ",""," "," "," "]
[" "," ","","其他措施项目 ",""," "," "," "]
["20","031302007019","","高层施工增加费"," ","项","1","27.30"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","专业措施项目 ",""," "," "," "]
["21","031301001019","","吊装加固"," ","项","0"," "]
["22","031301002019","","金属抱杆安装拆除、移位"," ","项","0"," "]
["23","031301003019","","平台铺设、拆除"," ","项","0"," "]
["24","031301004019","","顶升、提升装置"," ","项","0"," "]
["25","031301005019","","大型设备专用机具"," ","项","0"," "]
["26","031301006019","","焊接工艺评定"," ","项","0"," "]
["27","031301007019","","胎（模）具制作、安装、拆除"," ","项","0"," "]
["28","031301008019","","防护棚制作安装拆除"," ","项","0"," "]
["29","031301009019","","特殊地区施工增加"," ","项","0"," "]
["30","031301010019","","安装与生产同时进行施工增加"," ","项","0"," "]
["31","031301011019","","在有害身体健康环境中施工增加"," ","项","0"," "]
["32","031301012019","","工程系统检测、检验"," ","项","0"," "]
["33","031301013019","","设备、管道施工的安全、防冻和焊接保护"," ","项","0"," "]
["34","031301014019","","焦炉烘炉、热态工程"," ","项","0"," "]
["35","031301015019","","管道安拆后的充气保护"," ","项","0"," "]
["36","031301016019","","隧道内施工的通风、供水、供气、供电、照明及通讯设施"," ","项","0"," "]
["37","031301017019","","脚手架搭拆"," ","项","1","5495.85"]
["38","031301018019","","其他措施"," ","项","0"," "]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","分部小计 ",""," "," "," "]
["合    计","","","","","","",""]

{"sheet":"K.2 承包人提供主要材料和工程设备一览表(表-20)【B~2","index":8,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,10],[2,0,2,1],[2,5,2,6],[3,0,3,1],[3,5,3,6],[4,0,4,1],[4,5,4,6],[5,0,5,1],[5,5,5,6],[6,0,6,1],[6,5,6,6]],"flags":["formulas_cached_only"]}
[" 承包人提供主要材料和工程设备一览表\r\n（适用造价信息差额调整法）","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【弱电工程】","","","","标段：/","","","",""]
["序号","","名称、规格、型号","单位","数量","风险系数%","","基准单价(元)","招标控制单价(元)","发承包人确认单价(元)","备注"]
["1","","脚手架钢材","kg","102.349"," ",""," ","5.04"," "," "]
["2","","锯材 综合","m3","0.179"," ",""," ","2065.42"," "," "]
["3","","其他材料费","元","254.298"," ",""," ","1.22"," "," "]
["4","","柴油(机械)","L","12.46"," ",""," ","7.29"," "," "]

{"sheet":"F.1 分部分项工程和单价措施项目清单与计价表(表-08)~3","index":9,"n_rows":91,"n_cols":12,"rows_kept":91,"merged":[[0,0,0,11],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,11],[2,0,4,0],[2,1,4,2],[2,3,4,3],[2,4,4,4],[2,5,4,5],[2,6,4,6],[2,7,2,11],[3,7,4,7],[3,8,4,8],[3,9,3,11],[5,1,5,2],[5,3,5,4],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,1,15,2],[16,1,16,2],[17,1,17,2],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2],[36,1,36,2],[37,1,37,2],[38,1,38,2],[39,1,39,2],[40,1,40,2],[41,1,41,2],[42,1,42,2],[43,1,43,2],[44,1,44,2],[45,1,45,2],[46,1,46,2],[47,1,47,2],[48,1,48,2],[49,1,49,2],[50,1,50,2],[51,1,51,2],[52,1,52,2],[53,1,53,2],[54,1,54,2],[55,1,55,2],[56,1,56,2],[57,1,57,2],[58,1,58,2],[59,1,59,2],[60,1,60,2],[61,1,61,2],[62,1,62,2],[63,1,63,2],[64,1,64,2],[64,3,64,4],[65,1,65,2],[65,3,65,4],[66,1,66,2],[66,3,66,4],[67,1,67,2],[68,1,68,2],[68,3,68,4],[69,1,69,2],[69,3,69,4],[70,1,70,2],[71,1,71,2],[72,1,72,2],[73,1,73,2],[74,1,74,2],[75,1,75,2],[76,1,76,2],[77,1,77,2],[78,1,78,2],[79,1,79,2],[80,1,80,2],[81,1,81,2],[82,1,82,2],[83,1,83,2],[84,1,84,2],[85,1,85,2],[86,1,86,2],[87,1,87,2],[88,1,88,2],[88,3,88,4],[89,1,89,2],[89,3,89,4],[90,0,90,7]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表","","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【给排水工程】","","","","标段：/","","","","",""]
["序号"," 项目编码 ","","项目名称","项目特征描述","计量\r\n单位","工程量","金额（元）","","","",""]
["","","","","","","","综合单价","合价","其中","",""]
["","","","","","","","","","定额人工费","定额机械费","暂估价"]
[" "," ","","给排水工程 ",""," "," "," "," "," "," "," "]
["1","030601002003","","压力表","1.名称：压力表 就地\n2.包含取源部件、仪表接头、压力表表弯等附件\n3.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","40","48.73"]
["2","030817008007","","刚性防水套管 DN50","1.名称：刚性防水套管制作安装\n2.材质：碳钢\n3.规格：DN80\n4.填料材质：满足设计及规范要求，并综合考虑\n5.套管直径为被穿管道直径\n6.其它：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","380","82.46"]
["3","030817008008","","刚性防水套管 DN100","1.名称：刚性防水套管制作安装\n2.材质：碳钢\n3.规格：DN100\n4.填料材质：满足设计及规范要求，并综合考虑\n5.套管直径为被穿管道直径\n6.其它：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","68","82.46"]
["4","031001006041","","排水管H型管件","1.安装部位：室内\n2.介质：污水\n3.材质、规格：塑料\n4.连接形式：粘接\n5.其他：满足设计及规范要求","个","192","8.26"]
["5","031001006042","","直埋PP-R热水管 DN15","1.安装部位：综合考虑\n2.输送介质：给水（热水）\n3.材质：塑料\n4.型号、规格：DN15\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，管卡固定、临时封堵、配合隐蔽、水压试验及水冲洗、划线标示\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","1093.4","8.90"]
["6","031001006043","","直埋PP-R冷水管 DN15 ","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：塑料\n4.型号、规格：DN15\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，管卡固定、临时封堵、配合隐蔽、水压试验及水冲洗、划线标示\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","1374.4","17.79"]
["7","031001006044","","直埋PP-R热水管 DN20","1.安装部位：综合考虑\n2.输送介质：给水（热水）\n3.材质：塑料\n4.型号、规格：DN20\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，管卡固定、临时封堵、配合隐蔽、水压试验及水冲洗、划线标示\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","438.8","8.90"]
["8","031001006045","","直埋PP-R冷水管 DN20 ","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：塑料\n4.型号、规格：DN20\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，管卡固定、临时封堵、配合隐蔽、水压试验及水冲洗、划线标示\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","1301.2","20.72"]
["9","031001006046","","PP-R热水管 DN15","1.安装部位：综合考虑\n2.输送介质：给水（热水）\n3.材质：PPR管\n4.型号、规格：DN15\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","970.8","8.90"]
["10","031001006047","","PP-R冷水管 DN15 ","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：PPR管\n4.型号、规格：DN15\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","617.76","8.90"]
["11","031001006048","","管井PP-R冷水管 DN15","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：PPR管\n4.型号、规格：DN15\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","1.4","8.90"]
["12","031001006049","","PP-R热水管 DN20","1.安装部位：综合考虑\n2.输送介质：给水（热水）\n3.材质：PPR管\n4.型号、规格：DN20\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","337.28","8.90"]
["13","031001006050","","PP-R冷水管 DN20 ","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：PPR管\n4.型号、规格：DN20\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","2864.58","16.63"]
["14","031001006051","","管井PP-R冷水管 DN20","1.安装部位：综合考虑\n2.输送介质：给水（冷水）\n3.材质：PPR管\n4.型号、规格：DN20\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","809.6","8.90"]
["15","031001006052","","管井PP-R冷水管 DN40","1.安装部位：管井\n2.输送介质：给水（冷水）\n3.材质：PPR管\n4.型号、规格：DN40\n5.连接方式：热熔连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","33.3","8.90"]
["16","031001006053","","UPVC冷凝水管 DN50 ","1.安装部位：室内（综合）\n2.输送介质：冷凝水\n3.材质：UPVC冷凝水管\n4.型号、规格：DN50\n5.连接方式：粘接                        \n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","1465.9","8.90"]
["17","031001006054","","普通PVC-U排水管 DN50 ","1.安装部位：室内\n2.输送介质：污水、废水\n3.材质：UPVC实壁排水管\n4.型号、规格：DN50\n5.连接方式：粘接\n6.通气帽、检查口、止水环、H型管件、存水弯等材料综合考虑在单价内\n7.通球、灌水试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","896.88","8.90"]
["18","031001006055","","普通PVC-U排水管 DN75 ","1.安装部位：室内\n2.输送介质：污水、废水\n3.材质：UPVC实壁排水管\n4.型号、规格：DN75\n5.连接方式：粘接\n6.通气帽、检查口、止水环、H型管件、存水弯等材料综合考虑在单价内\n7.通球、灌水试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","867.28","8.90"]
["19","031001006056","","加厚型PVC-U排水管 DN100","1.安装部位：室内\n2.输送介质：污水、废水\n3.材质：UPVC实壁排水管\n4.型号、规格：DN100\n5.连接方式：粘接\n6.通气帽、检查口、止水环、H型管件、存水弯等材料综合考虑在单价内\n7.通球、灌水试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","189.1","8.90"]
["20","031001006057","","普通PVC-U排水管 DN100 ","1.安装部位：室内\n2.输送介质：污水、废水\n3.材质：UPVC实壁排水管\n4.型号、规格：DN100\n5.连接方式：粘接\n6.通气帽、检查口、止水环、H型管件、存水弯等材料综合考虑在单价内\n7.通球、灌水试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","2333.26","37.65"]
["21","031001006058","","普通PVC-U雨水管 DN100 ","1.安装部位：室内\n2.输送介质：雨水\n3.材质：PVC-U\n4.型号、规格：DN100\n5.连接方式：粘接\n6.包含切管、组对、粘接，管道及管件安装，灌水试验\n7.通球试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","707.5","8.90"]
["22","031001006059","","加厚型PVC-U雨水管 DN100 ","1.安装部位：室内\n2.输送介质：雨水\n3.材质：PVC-U\n4.型号、规格：DN100\n5.连接方式：粘接\n6.包含切管、组对、粘接，管道及管件安装，灌水试验\n7.通球试验按设计要求\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","10.24","8.90"]
["23","031001007010","","管井衬塑钢管 DN40","1.安装部位：管井\n2.输送介质：给水（冷水）\n3.材质：衬塑钢管\n4.型号、规格：DN40\n5.连接方式：丝扣连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","17.2","10.24"]
["24","031001007011","","管井衬塑钢管 DN50","1.安装部位：管井\n2.输送介质：给水（冷水）\n3.材质：衬塑钢管\n4.型号、规格：DN50\n5.连接方式：丝扣连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","19.6","10.24"]
["25","031001007012","","管井衬塑钢管 DN65","1.安装部位：管井\n2.输送介质：给水（冷水）\n3.材质：衬塑钢管\n4.型号、规格：DN65\n5.连接方式：丝扣连接\n6.包含切管、组对、预热、熔接，管道及管件安装，水压试验及水冲洗\n7.给水管道消毒符合设计及规范\n8.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m","124","10.24"]
["26","031002001009","","管道支架","1.名称：管道支架\n2.材质:碳钢(型钢综合)\n3.除锈级别 ：轻锈\n4.油漆品种：管道支架除锈后调和漆二道\n5.涂刷遍数、漆膜厚度：详设计\n6.标志色方式、品种：详设计\n7.未尽事宜详设计图纸，并须符合国家现行相关规范及标准","Kg","44.11","11.94"]
["27","031002003030","","镀锌钢套管 DN25","1.名称：钢套管制作安装\n2.材质：镀锌\n3.规格：套管公称直径DN25，介质管道公称直径DN15\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","248","16.96"]
["28","031002003031","","镀锌钢套管 DN32","1.名称：钢套管制作安装\n2.材质：镀锌\n3.规格：套管公称直径DN32，介质管道公称直径DN20\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","724","16.96"]
["29","031002003032","","管井镀锌钢套管 DN65","1.名称：钢套管制作安装\n2.材质：镀锌\n3.规格：套管公称直径DN65，介质管道公称直径DN40\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","8","16.96"]
["30","031002003033","","管井镀锌钢套管 DN80","1.名称：钢套管制作安装\n2.材质：镀锌\n3.规格：套管公称直径DN80，介质管道公称直径DN50\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","8","16.96"]
["31","031002003034","","管井镀锌钢套管 DN100","1.名称：钢套管制作安装\n2.材质：镀锌\n3.规格：套管公称直径DN100，介质管道公称直径DN65\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","42","16.96"]
["32","031002003035","","阻火圈 DN100","1.名称：阻火圈\n2.规格：DN100\n3.填料材质：满足设计和规范要求\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","600","18.69"]
["33","031002003036","","成品管卡 DN15","1.名称、类型：成品管卡\n2.材质：详设计\n3.型号、规格：DN15\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","4268","2.82"]
["34","031002003037","","成品管卡 DN20","1.名称、类型：成品管卡\n2.材质：详设计\n3.型号、规格：DN20\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","6214","2.82"]
["35","031002003038","","成品管卡 DN50","1.名称、类型：成品管卡\n2.材质：详设计\n3.型号、规格：DN50\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","1045","2.82"]
["36","031002003039","","成品管卡 DN80","1.名称、类型：成品管卡\n2.材质：详设计\n3.型号、规格：DN80\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","371","2.82"]
["37","031002003040","","成品管卡 DN100","1.名称、类型：成品管卡\n2.材质：详设计\n3.型号、规格：DN100\n4.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","1314","2.82"]
["38","031003001022","","管井Y型过滤器 DN40","1.名称：截止阀\n2.材质：详设计\n3.规格、压力等级：DN40 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","20","23.43"]
["39","031003001023","","管井电磁阀 DN15","1.名称：螺纹电磁阀\n2.材质：详设计\n3.规格、压力等级：DN15 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","2","23.43"]
["40","031003001024","","管井电磁阀 DN20","1.名称：螺纹电磁阀\n2.材质：详设计\n3.规格、压力等级：DN20 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","188","23.43"]
["41","031003001025","","截止阀 DN20","1.名称：截止阀\n2.材质：详设计\n3.规格、压力等级：DN20 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","188","23.43"]
["42","031003001026","","管井截止阀 DN20","1.名称：截止阀\n2.材质：详设计\n3.规格、压力等级：DN20 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","188","23.43"]
["43","031003001027","","管井截止阀 DN40","1.名称：截止阀\n2.材质：详设计\n3.规格、压力等级：DN40 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：管井\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","52","23.43"]
["44","031003001028","","管井截止阀 DN15","1.名称：截止阀\n2.材质：详设计\n3.规格、压力等级：DN15 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：管井\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","2","23.43"]
["45","031003001029","","管井止回阀 DN15","1.名称：止回阀\n2.材质：详设计\n3.规格、压力等级：DN15 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：管井\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","2","23.43"]
["46","031003001030","","管井止回阀 DN20","1.名称：止回阀\n2.材质：详设计\n3.规格、压力等级：DN20 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：管井\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","188","23.43"]
["47","031003001031","","管井自动排气阀 DN15","1.名称：自动排气阀\n2.材质：全铜\n3.规格、压力等级：DN15 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：管井\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","2","23.43"]
["48","031003001032","","自动排气阀 DN15","1.名称：自动排气阀\n2.材质：全铜\n3.规格、压力等级：DN15 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","4","37.01"]
["49","031003006003","","可调式减压阀 DN40","1.名称：减压阀\n2.材质：详设计\n3.规格、压力等级：DN40 压力等级详设计\n4.连接形式：螺丝连接\n5.安装部位：详设计\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","组","24","86.78"]
["50","031004004003","","不锈钢洗菜盆\n","1.名称：洗菜盆\n2.材质：不锈钢\n3.规格、类型：详设计\n4.组装形式：详设计\n5.包含打螺栓孔、托架安装、冷热水龙头、洗涤盆及附件安装、与上下水管连接、试水\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求\n","组","188","115.37"]
["51","031004006004","","蹲式大便器 瓷低水箱","1.名称：蹲式大便器 瓷低水箱\n2.规格、类型：详设计\n3.组装方式：含本体、水箱及配件、角阀等所有附配件成套制作安装\n4.蹲便器、水箱和阀门均为同一品牌的配套产品\n5.包含打螺栓孔，大便器、水箱及附件安装，与上下水管连接，试水\n6.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","组","188","160.65"]
["52","031004014012","","管井水龙头 DN15","1.名称：水龙头\n2.型号、规格：DN15\n3.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","2","4.21"]
["53","031002003041","","塑料套管制作安装 DN75","1.名称：塑料套管制作安装\n2.材质：塑料\n3.规格：DN75\n4.填料材质：满足设计及规范要求，并综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","624","16.96"]
["54","031004014013","","给水堵头 DN15","1.名称：给水堵头 \n2.型号、规格：DN15\n3.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","1316","2.82"]
["55","031004014014","","地漏 DN50","1.名称：直通式地漏\n2.材质：综合考虑\n3.型号、规格：DN50\n4.其他：直通式地漏，满足规范及设计任务书\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","284","24.21"]
["56","031004014015","","洗衣机地漏 DN50","1.名称：直通式地漏\n2.材质：综合考虑\n3.型号、规格：DN50\n4.其他：直通式地漏，满足规范及设计任务书\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","188","24.21"]
["57","031004014016","","侧墙雨水斗 DN100","1.名称：侧墙雨水斗\n2.型号、规格：DN100\n3.安装位置：屋面\n4.材质：综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","个","16","46.11"]
["58","040101002003","","机械挖沟槽土方","1.土方类别：综合考虑\n2.挖土深度：综合考虑\n3.开挖方式：机械挖\n4.场内运输方式、距离、堆置：综合考虑\n5.其他：满足设计、招标文件、技术标准和要求、相关图集、现行施工及验收规范等相关要求","m3","125.96","8.07"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","单价措施项目清单 ",""," "," "," "]
[" "," ","","其他措施项目 ",""," "," "," "]
["59","031302007020","","高层施工增加费"," ","项","1","27.30"]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","专业措施项目 ",""," "," "," "]
["60","031301001020","","吊装加固"," ","项","0"," "]
["61","031301002020","","金属抱杆安装拆除、移位"," ","项","0"," "]
["62","031301003020","","平台铺设、拆除"," ","项","0"," "]
["63","031301004020","","顶升、提升装置"," ","项","0"," "]
["64","031301005020","","大型设备专用机具"," ","项","0"," "]
["65","031301006020","","焊接工艺评定"," ","项","0"," "]
["66","031301007020","","胎（模）具制作、安装、拆除"," ","项","0"," "]
["67","031301008020","","防护棚制作安装拆除"," ","项","0"," "]
["68","031301009020","","特殊地区施工增加"," ","项","0"," "]
["69","031301010020","","安装与生产同时进行施工增加"," ","项","0"," "]
["70","031301011020","","在有害身体健康环境中施工增加"," ","项","0"," "]
["71","031301012020","","工程系统检测、检验"," ","项","0"," "]
["72","031301013020","","设备、管道施工的安全、防冻和焊接保护"," ","项","0"," "]
["73","031301014020","","焦炉烘炉、热态工程"," ","项","0"," "]
["74","031301015020","","管道安拆后的充气保护"," ","项","0"," "]
["75","031301016020","","隧道内施工的通风、供水、供气、供电、照明及通讯设施"," ","项","0"," "]
["76","031301017020","","脚手架搭拆"," ","项","1","294.18"]
["77","031301018020","","其他措施"," ","项","0"," "]
[" "," ","","分部小计 ",""," "," "," "]
[" "," ","","分部小计 ",""," "," "," "]
["合    计","","","","","","",""]

{"sheet":"K.2 承包人提供主要材料和工程设备一览表(表-20)【B~3","index":10,"n_rows":7,"n_cols":11,"rows_kept":7,"merged":[[0,0,0,10],[1,0,1,1],[1,2,1,5],[1,6,1,8],[1,9,1,10],[2,0,2,1],[2,5,2,6],[3,0,3,1],[3,5,3,6],[4,0,4,1],[4,5,4,6],[5,0,5,1],[5,5,5,6],[6,0,6,1],[6,5,6,6]],"flags":["formulas_cached_only"]}
[" 承包人提供主要材料和工程设备一览表\r\n（适用造价信息差额调整法）","","","","","","","","","",""]
["工程名称：","","遂宁市安居区东城二期棚户区改造项目\\B-03-10地块1号楼【给排水工程】","","","","标段：/","","","",""]
["序号","","名称、规格、型号","单位","数量","风险系数%","","基准单价(元)","招标控制单价(元)","发承包人确认单价(元)","备注"]
["1","","脚手架钢材","kg","6.111"," ",""," ","5.04"," "," "]
["2","","锯材 综合","m3","0.011"," ",""," ","2065.42"," "," "]
["3","","其他材料费","元","15.568"," ",""," ","1.22"," "," "]
["4","","柴油(机械)","L","50.771"," ",""," ","7.29"," "," "]